; Control Command
BDM_NOP            EQU     0000h
BDM_GO             EQU     0C00h

; Memory Access
BDM_READ_MEM       EQU     1900h
BDM_WRITE_MEM      EQU     1800h
BDM_DUMP_MEM       EQU     1D00h
BDM_FILL_MEM       EQU     1C00h
; Sizing Field of Memory Access
BDM_BYTE           EQU     00h
BDM_WORD           EQU     40h
BDM_LONG           EQU     80h

; A/D Register Access
BDM_READ_REG       EQU     2180h
BDM_WRITE_REG      EQU     2080h
BDM_ADDR_REG       EQU     8

; Debug Command
BDM_READ_DEBUG     EQU     2D80h
BDM_WRITE_DEBUG    EQU     2C80h
; Debug Register
BDM_CSR            EQU     00h
BDM_AABR           EQU     06h
BDM_TDR            EQU     07h
BDM_PBR            EQU     08h
BDM_PBMR           EQU     09h
BDM_ABHR           EQU     0Ch
BDM_ABLR           EQU     0Dh
BDM_DBR            EQU     0Eh
BDM_DBMR           EQU     0Fh

; Control Register Access
BDM_READ_CTRL      EQU     2980h
BDM_WRITE_CTRL     EQU     2880h
; Control Register
BDM_VBR            EQU     0801h
BDM_SR             EQU     080Eh
BDM_PC             EQU     080Fh
