In the window, you can display trace frames in bus-cycle, 
assembly and source forms.


EasyPack/SLD has 3 event settings. That is Event1, 
Event2 and Event3. Event1 and Event2 are bus event 
which have multiple settings for address, data and 
cycle status. Event3 is an event level triggered 
by an external hardware signal. 