The status combo is five processor status code 
(as defined in the table below) to specify status 
code to be matched as part of the event condition.


S : Instruction

F : Program memory read

R : Data memory read

W : Data memory write

AK: Interrupt acknowledge
