Display or edit bit memory from the bit memory window. 


Bit memory is displayed in 2 regions. 


The left is the hexadecimal memory address (from 00~F0H). 


The right is the bit memory status (0 or 1).