In the Filter Tab you can --

set the conditions of displayed trace or the conditions of tracing. 
  The default is Display. 

2. Three kinds of address/data mode can be chose:
	Range allows you to enter an  address/data range with start address and end address. 
	Multiple allows you to enter up to 10 address/data (wildcard is not allowed in this case) separated with comma. 
	Wildcard allows a wildcard address/data.
The status combo is five processor status code (as defined in the table below) to specify status code to be matched as part of the event condition.
Code	Status
S	Instruction
F	Program memory read
R	Data memory read
W	Data memory write
AK	Interrupt acknowledge
Defining A Trace Buffer Trigger
To define a trace buffer trigger, do any of the following:
· From the Group menu choose the Trace command and switch to the Trigger tab. 
· From the Trace menu in the Trace window, choose the Trigger command. 
· From the shortcut menu in the Trace window, choose the Trigger command.
 
