when you select Event3 only the High/Low options are available. 
The count options will be greyed. 


· High: specify the signal High level to be
matched at the EXT TRIGGER INPUT for Event3. 


· Low: specify the signal Low level to be
matched at the EXT TRIGGER INPUT
for Event3. It’s the default.

 