EasyPack 8052F has 3 event settings. 
That is Event1, Event2 and Event3. 


Event1 and Event2 
are bus event which have multiple settings for address, 
data and cycle status. 


Event3 is an event level triggered 
by an external hardware signal. 

