The status combo is five processor status code 
(as defined in the table below) to specify status 
code to be matched as part of the event condition.


 
S : Instruction.
  
 
 
 F : Program memory read.
  
 
R : Data memory read.
 
 
 
 W : Data memory write.
  
 
 
 AK: Interrupt acknowledge.
