Rem ***** Set parallel port communication address 200
p:200

rem  ***** Emulation mode default is 80C186XL if no T option. ******
t:186XL
rem t:188XL
rem t:188EA
rem t:186EA
rem t:186EB
rem t:188EB
rem t:186EC
rem t:188EC

rem ***** Enable Function Test *****
rem F:1

rem ***** Enable Diagnosis *****
rem D:1

rem ***** Start to Max view port *****
rem m:1

rem ***** Start to execute include file Start.inc
rem i:start.inc

rem ***** Reserve address for software breakpoint. *****
rem V:0:1000

rem ***** Define target CPU as non-stop free running when MICEview is invoked
rem r:y
