*SPA_COVER
*Linking MICE
Retry
*80386,A
Protecting Mode
Real Mode
*8052,A
Program Memory
External Data
*SetClear,A
Set
CLear
*OnOff,A
ON
OFF
*Delay,A
BACKWARD
CENTER
FORWARD
COUNT
*ListFormat,A
Instruction
Source
Mixed
Module
Raw Data
*OUoption,A
Screen Layout
Softkey Definition
*YListOptions,A
ALL
GLOBAL
MODULE
*BreakOperation,A
SET
RESET
CLEAR
ENABLE
DISABLE
*LevelOperation,A
SET
CLEAR
CLEAR ALL
*LAM2TraceCycle,A
SET
CLEAR
ENABLE
DISABLE
*MonitorType,A
BYTE
WORD
LONG
*TRACEMODE,A
BAckward
Center
Forward
*MapAttrHEMM,A
I
IR
E
ER
G
*MapAttrEMM,A
I
IR
E
*MapAttr8688,A
I
IR
ID
E
ER
ED
G
*MapOptions,A
All External
Program
Data
*Operation,A
Set
Disable
Enable
*EventAddrLAM2,A
Range
Single
Wildcard
*EventAddrLAM,A
Single
Wildcard
*Status,A
  S  : Instruction Fetch
  R  : Read Data from Memory
  W  : Write Data to Memory
  I  : Read I/O
  O  : Write I/O
  AK : Interrupt Acknowledge
  H  : Halt
*TriggerOperation,A
Set
Show
Clear
*EventSequence,A
EV1
EV2
EV3
EV1 Then EV2
EV1 Then EV3
EV2 Then EV1
EV2 Then EV3
EV3 Then EV1
EV3 Then EV2
EV1 Then EV2 Then EV3
EV1 Then EV3 Then EV2
EV2 Then EV1 Then EV3
EV2 Then EV3 Then EV1
EV3 Then EV1 Then EV2
EV3 Then EV2 Then EV1
EV1 And EV2
EV1 And EV3
EV2 And EV3
EV1 And EV2 And EV3
EV1 Or EV2
EV1 Or EV3
EV2 Or EV3
EV1 Or EV2 Or EV3
EV1 And EV2 Then EV3
EV1 And EV3 Then EV2
EV2 And EV3 Then EV1
EV1 Or EV2 Then EV3
EV1 Or EV3 Then EV2
EV2 Or EV3 Then EV1
*TriggerAction,A
Break
Run
*TriggerMode,A
Backward
Forward
Center
Delay
*LAM2Seq0,A
EV1
NOT EV1
EV2
NOT EV2
EV3
NOT EV3
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq1,A
EV2
NOT EV2
EV3
NOT EV3
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq2,A
EV1
NOT EV1
EV3
NOT EV3
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq3,A
EV3
NOT EV3
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq4,A
EV1
NOT EV1
EV2
NOT EV2
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq5,A
EV2
NOT EV2
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq6,A
EV1
NOT EV1
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq7,A
EV4
NOT EV4
EV5
NOT EV5
*LAM2Seq8,A
EV1
NOT EV1
EV2
NOT EV2
EV3
NOT EV3
EV5
NOT EV5
*LAM2Seq9,A
EV2
NOT EV2
EV3
NOT EV3
EV5
NOT EV5
*LAM2Seq10,A
EV1
NOT EV1
EV3
NOT EV3
EV5
NOT EV5
*LAM2Seq11,A
EV3
NOT EV3
EV5
NOT EV5
*LAM2Seq12,A
EV1
NOT EV1
EV2
NOT EV2
EV5
NOT EV5
*LAM2Seq13,A
EV2
NOT EV2
EV5
NOT EV5
*LAM2Seq14,A
EV1
NOT EV1
EV5
NOT EV5
*LAM2Seq15,A
EV5
NOT EV5
*LAM2Seq16,A
EV1
NOT EV1
EV2
NOT EV2
EV3
NOT EV3
EV4
NOT EV4
*LAM2Seq17,A
EV2
NOT EV2
EV3
NOT EV3
EV4
NOT EV4
*LAM2Seq18,A
EV1
NOT EV1
EV3
NOT EV3
EV4
NOT EV4
*LAM2Seq19,A
EV3
NOT EV3
EV4
NOT EV4
*LAM2Seq20,A
EV1
NOT EV1
EV2
NOT EV2
EV4
NOT EV4
*LAM2Seq21,A
EV2
NOT EV2
EV4
NOT EV4
*LAM2Seq22,A
EV1
NOT EV1
EV4
NOT EV4
*LAM2Seq23,A
EV4
NOT EV4
*LAM2Seq24,A
EV1
NOT EV1
EV2
NOT EV2
EV3
NOT EV3
*LAM2Seq25,A
EV2
NOT EV2
EV3
NOT EV3
*LAM2Seq26,A
EV1
NOT EV1
EV3
NOT EV3
*LAM2Seq27,A
EV3
NOT EV3
*LAM2Seq28,A
EV1
NOT EV1
EV2
NOT EV2
*LAM2Seq29,A
EV2
NOT EV2
*LAM2Seq30,A
EV1
NOT EV1
*LAM2TrigLogic,A
AND
OR
*LAM2TLevelOp,A
Set
Show
Clear
*LAM2TLevelNo,A
A
B
C
D
E
F
G
H
*LAM2TLevelTrace,A
ON
OFF
*LAM2TLevelTimer,A
ON
OFF
*LAM2TriggerOperation,A
Set
Show
Clear
*LAM2TriggerTrace,A
ON
OFF
*LAM2TriggerTimer,A
ON
OFF
*LAM2TriggerAction,A
Break
Run
*LAM2TriggerMode,A
Backward
Forward
Center
Delay
