rem Using COM2 serial port, 9600 baud, 8 data-bit, no parity 
s:com2,19200,8,n 

rem Using parallel port and the port address as 200 
rem p:200

rem Set MAX COMMAND viewport when enter USD3
rem m:1

rem Logging MICE communication data in file log.1 
o:log.1 

rem Keep MICE free-running when enter USD-III
rem r:y

rem Disable SW breakpoint
rem v:n
rem Assign SW breakpoint trap handler location at location 2000
rem v:2000

rem Execute the include file, test1.inc, when enter USD-III
rem i:test1.inc
 