S:com2,19200

rem Using communication port as parallel port 0x200 
rem P:100
 
rem Set MAX CODE viewport when starting USD3 
rem m:1 
 
rem Logging MICE communication data in file log.1 
o:log.1 
 
rem Keep MICE free-running when enter USD-III 
rem r:y 
 
rem Disable SW breakpoint 
rem v:n 
 
rem Assign SW breakpoint trap handler location at location 2000 
rem v:400
 
rem Include file to be executed on initial startup 
rem I:startup.inc 
