            How to use those demo files

1) Threadx demo for EV40 Board(CPU = AT91M40800)
 a.Start JediView's "Configuration for ARM", set like following:
   Maker: ATMEL
   Target CPU: ARM7TDMI-AT91M40400
   Endian: little Endian
   Use Initialize file: checked
   select "micev40_em.inc" in directory "threadx v4.0 for EV40 at 0x02000000(little)"
 b.Start JediView for ARM, load demo.out in directory "threadx v4.0 for EV40 at 0x02000000(little)"
   then can go ,stop,set breakpoint,watch task info and so on.
 c.Notes:
   The start address will be 0x02000000.
   using little endian mode.

2) Threadx demo for EV4510 Board(CPU = S3c4510B)
 a.Start JediView's "Configuration for ARM", set like following:
   Maker: SamSung
   Target CPU: ARM7TDMI-S3c4510b
   Endian: big Endian
   Use Initialize file: checked
   select "ev4510_0.inc" in directory "threadx v4.0 for ev4510 at 0x0(big)"
 b.Start JediView for ARM, load demo.out in directory "threadx v4.0 for ev4510 at 0x0(big)"
   then can go ,stop,set breakpoint,watch task info and so on.
 c.Notes:
   The start address will be 0x00000000.
   using big endian mode.