<SETUP CpuVendor="Samsung" CpuChip="S3C2510" FlashVendor="AdvancedMicroDevices" FlashChip="AM29LV160B/DB" RamAddress="0x0" RamSize="0x400000" FlashAddress="0x80000000" FlashSize="0x200000" CpuType="ARM940T" CpuFamily="ARM" Register7="0x3" ManufacturersCode="1" DeviceID="0X2249" INIFile="" FailMask="0x0" CpuEndian="Little" LoadFileLE="arm7.bin" LoadFileBE="arm7be.bin" Regcount="0x24" Seccount="0x23" FlashWidth="0x10" FlashChipsPerSector="0x1">
    <Regcount Regcount="0x24">
        <Sim Register="0xf0000008" Address="0xf0000008" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0xf000000c" Address="0xf000000c" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0xf0140008" Address="0xf0140008" Value="0xffffffff" Default="0x0" Width="32" />
        <Sim Register="0xf014000c" Address="0xf014000c" Value="0x8000003f" Default="0x0" Width="32" />
        <Sim Register="0x40108d74" Address="0x40108d74" Value="0x09e4f580" Default="0x0" Width="32" />
        <Sim Register="0x40108d78" Address="0x40108d78" Value="0x07ed6b40" Default="0x0" Width="32" />
        <Sim Register="0xf0020004" Address="0xf0020004" Value="0x00000001" Default="0x0" Width="32" />
        <Sim Register="0xf0020008" Address="0xf0020008" Value="0x00000020" Default="0x0" Width="32" />
        <Sim Register="0x40108d74" Address="0x40108d74" Value="0x09e4f580" Default="0x0" Width="32" />
        <Sim Register="0x40108d78" Address="0x40108d78" Value="0x07ed6b40" Default="0x0" Width="32" />
        <Sim Register="0xf0020008" Address="0xf0020008" Value="0x0000081a" Default="0x0" Width="32" />
        <Sim Register="0xf0020000" Address="0xf0020000" Value="0x00058aac" Default="0x0" Width="32" />
        <Sim Register="0xf0020004" Address="0xf0020004" Value="0x00000002" Default="0x0" Width="32" />
        <Sim Register="0xf0020004" Address="0xf0020004" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0xf0020004" Address="0xf0020004" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0xf002000c" Address="0xf002000c" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0xf0010000" Address="0xf0010000" Value="0x850a1111" Default="0x0" Width="32" />
        <Sim Register="0xf0010004" Address="0xf0010004" Value="0x8514e488" Default="0x0" Width="32" />
        <Sim Register="0xf0010008" Address="0xf0010008" Value="0xc594e488" Default="0x0" Width="32" />
        <Sim Register="0xf001000c" Address="0xf001000c" Value="0xc58ae001" Default="0x0" Width="32" />
        <Sim Register="0xf0010010" Address="0xf0010010" Value="0xc58ae001" Default="0x0" Width="32" />
        <Sim Register="0xf0010014" Address="0xf0010014" Value="0xc58ae001" Default="0x0" Width="32" />
        <Sim Register="0xf0010018" Address="0xf0010018" Value="0x850a1111" Default="0x0" Width="32" />
        <Sim Register="0xf001001c" Address="0xf001001c" Value="0xc58ae011" Default="0x0" Width="32" />
        <Sim Register="0xf0010020" Address="0xf0010020" Value="0x006db6db" Default="0x0" Width="32" />
        <Sim Register="0xf0010024" Address="0xf0010024" Value="0x00ff0000" Default="0x0" Width="32" />
        <Sim Register="0x40000000" Address="0x40000000" Value="0x40000050" Default="0x0" Width="32" />
        <Sim Register="0x40000004" Address="0x40000004" Value="0x00000448" Default="0x0" Width="32" />
        <Sim Register="0x40000008" Address="0x40000008" Value="0x00000458" Default="0x0" Width="32" />
        <Sim Register="0x4000000c" Address="0x4000000c" Value="0x000004c0" Default="0x0" Width="32" />
        <Sim Register="0x40000010" Address="0x40000010" Value="0x000004d4" Default="0x0" Width="32" />
        <Sim Register="0x40000014" Address="0x40000014" Value="0x000004e8" Default="0x0" Width="32" />
        <Sim Register="0x40000018" Address="0x40000018" Value="0x000004ec" Default="0x0" Width="32" />
        <Sim Register="0x4000001c" Address="0x4000001c" Value="0x000004f0" Default="0x0" Width="32" />
        <Sim Register="0x40108d78" Address="0x40108d78" Value="0x07ed6b40" Default="0x0" Width="32" />
        <Sim Register="0xf0000000" Address="0xf0000000" Value="0x00000100" Default="0x0" Width="32" />
    </Regcount>
    <Seccount Seccount="0x23">
        <Sector1 Sector="1" Size="65536" />
    </Seccount>
    <CommandType name="AMD:LV8/16">
        <type name="AMD:LV8/16">
            <BUS width="8">
                <reset>
                    <item addr="0XAAA" data="0XF0" />
                </reset>
                <MC>
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X90" />
                    <item addr="0X00" data="READ" />
                </MC>
                <DID>
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X90" />
                    <item addr="0X01" data="READ" />
                </DID>
                <ChipErase>
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X80" />
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X10" />
                </ChipErase>
                <SectorErase>
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X80" />
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="WRITE" data="0X30" />
                </SectorErase>
                <Program>
                    <item addr="0XAAA" data="0XAA" />
                    <item addr="0X555" data="0X55" />
                    <item addr="0XAAA" data="0X00A0" />
                </Program>
            </BUS>
            <BUS width="16">
                <reset>
                    <item addr="0X555" data="0X00F0" />
                </reset>
                <MC>
                    <item addr="0X555" data="0XAAAA" />
                    <item addr="0X2AA" data="0X5555" />
                    <item addr="0X555" data="0X0090" />
                    <item addr="0X0000" data="READ" />
                </MC>
                <DID>
                    <item addr="0X555" data="0XAAAA" />
                    <item addr="0X2AA" data="0X5555" />
                    <item addr="0X555" data="0X0090" />
                    <item addr="0X01" data="READ" />
                </DID>
                <ChipErase>
                    <item addr="0X555" data="0XAA" />
                    <item addr="0X2AA" data="0X55" />
                    <item addr="0X555" data="0X80" />
                    <item addr="0X555" data="0XAA" />
                    <item addr="0X2AA" data="0X55" />
                    <item addr="0X555" data="0X10" />
                </ChipErase>
                <SectorErase>
                    <item addr="0X555" data="0XAA" />
                    <item addr="0X2AA" data="0X55" />
                    <item addr="0X555" data="0X80" />
                    <item addr="0X555" data="0XAA" />
                    <item addr="0X2AA" data="0X55" />
                    <item addr="WRITE" data="0X30" />
                </SectorErase>
                <Program>
                    <item addr="0X555" data="0X00AA" />
                    <item addr="0X2AA" data="0X0055" />
                    <item addr="0X555" data="0X00A0" />
                </Program>
            </BUS>
        </type>
    </CommandType>
    <Param FlashStart="0x80000000" FileStart="0x0" FileEnd="0x200000" />
</SETUP>
