  Thank for your interest on our JediView for PowerPC IDE software.
   Working with USB TAP in-circuit emulator, JediView for PPC can be used to debug Freescale PowerPC board.

USBTAP Features:
¡ñ Support JTAG, COP or BDM interface
¡ñ High-speed USB 2.0 download, plug and play without external power supply
¡ñ With the speed of loading code up to 1.6Mbps
¡ñ Can check and control the current status of the registers in processor and memory
¡ñ Flash memory programming
¡ñ Low voltage target support: 1.8~3.3V
¡ñ Seamlessly integrated with JediView or CodeWarrior Integrated Development Environment (IDE)

JediView for PowerPC Features:
¡ñ Support Freescale MPC8xx, MPC82xx, MPC83xx, MPC85xx, MPC5xx,MPC52xx
¡ñ Support C/C++ language and assembly programming-level debugging
¡ñ Debugging bootloader, Vxworks, Linux, uclinux etc
¡ñ Real-time debugging: single-step, free run, reset, software/hardware breakpoint and jump
¡ñ ¡¤Hardware Diagnostics to detect if there¡¯s any problem with CPU, RAM or Flash on the board
¡ñ Windows for CPU and registers, memory, variable and stack etc for checking and revising the data
¡ñ Watch window for adding custom register, memory address and variable
¡ñ In-circuit Flash programming, support more than 200 kinds of Flash. And user can add flash type by himself refer to our document.

If you have any problem,please mail to international.sales@micetek.com

JediView use guide:

1, Set up JediView software. Please enter JediView_PPC0.xx and click Setup.exe,
   then you can complete JediView installation.

2, USBTAP Driver Installation Manual :
--------------------------------------------------
                        Supported Devices:  Freescale USB TAP  Micetek USBTAP
       Supported Operating Systems:  Windows 2000         Windows XP

  Installation Instructions:
  Please note that the following procedures assume that the user has 
  installed JediView on C:\ root directory.

  2.1.  Launch a Windows command shell and change the driver directory:
        Start->Programs->Accessories->Command Prompt
        C:\Profiles\Username> cd \Jediview.PPC
        C:\JediView.PPC>cd ccs\drivers\usb

  2.2.  Unplug all USB TAPs from your machine

  2.3.  Install the driver with the setup command:
        C:\JediView.PPC\ccs\drivers\usb> setup

  2.4.  When you finish executing 2.3 step,please plug in USB TAP 

  2.5   The Found New Hardware Wizard will run, browse to usbtap.inf which is
        is located in the ccs/drivers/usb folder

  2.6,  You can find CodeWarrior USB TAP in system devices on Devices manager panel of your machine

3, Get JediView License
      Without a formal license or a demo license, you can't enable programming flash nor invoking the symbol
      table to trace and debug code in JediView.

   3.1   Get JediView evaluation License
         please refer to Chapter 3: Procedures of installing and registering JediView in       JediViewPPC_QuickStart_Engilsh.pdf or JediViewPPC_QuickStart_Chinese.pdf document.You need send ¡°regform.ini¡± to Micetek PowerPC technical support:  withoutend@micetek.com.cn or lls@micetek.com.cn. 
You will receive a demo license in one workday.  We can give you a two-week license for to evaluate JediView

   3.2   Get JediView official License
         please mail to international.sales@micetek.com

4, Install JediView License that you receive from micetek 
        Please copy the license.xml file, either in the installing disk or acquired from Micetek, to the" private" folder    in JediView installing directory. If your JediView is installed in C:\ root directory, then simply copy the license.xml file to C:\JediView.PPC\private directory to finish registration.Click the register.exe file in JediView installing directory, and a dialog box will pop up showing whether the registration is successful.

5, Use JediView and USB TAP to debug your PowerPC board
   please refer to JediViewPPC_QuickStart_Engilsh.pdf or JediViewPPC_QuickStart_Chinese.pdf
 
   Chapter 1, Introduce the USB TAP and JediView software;
   Chapter 2, Establish the developing and debugging environment for PowerPC;
   Chapter 3, Procedures of installing and registering JediView;
   Chapter 4, program Flash with JediView and USB TAP;
   Chapter 5, Debug the U-boot codes;
   Chapter 6, Debug the Linux codes;
   Chapter 7, Debug the Vxworks codes.

6,JediView for PowerPC and USB TAP support the following Freescale PowerPC processors:

   MPC52XX
   MPC5200 MPC5200B

   MPC5xx
   MPC533, MPC535, MPC555, MPC561, MPC563, MPC565

   MPC8XX 
   MPC823, MPC823E, MPC850, MPC852T, MPC853T, MPC855T,
   MPC857DSL, MPC857T, MPC859DSL, MPC860, MPC862,
   MPC866, MPC870, MPC875, MPC880, MPC885

   MPC82xx
   MPC8241, MPC8245, MPC8247, MPC8248, MPC8250, MPC8255,
   MPC8260, MPC8264, MPC8265, MPC8266, MPC8270, MPC8271, MPC8272,
   MPC8275, MPC8280

   MPC83XX 
   MPC8313E, MPC8314E, MPC8315E, 
   MPC8321E, MPC8323E, MPC8343E, MPC8347E, MPC8349E,
   MPC8358E, MPC8360E, MPC8377E, MPC8378E, MPC8379E

   MPC85XX 
   MPC8533E, MPC8540E, MPC8541E, MPC8543E, MPC8544E,
   MPC8545E, MPC8547E, MPC8548E, MPC8555E, MPC8560E, MPC8567E,
   MPC8568E, MPC8572E

Contact us:
Headquarter in Taiwan
Tel: 886-4-23026168 Fax: 886-4-23036268
Email: international.sales@micetek.com
http://www.micetek.com

