// An Example memory config file for Lite5200

reservedchar 0xBA

range    0x00000000 0x03FFFFFF 4 ReadWrite
reserved 0x04000000 0x7FFFFFFF

// reserve for XLB Arbiter problem
reserved 0xF00000c0 0xF00000ff

// reserve for ATADRIVE reg problem
reserved 0xF0003A50 0xF0003A83 

reserved 0xF0004100 0xFEFFFFFF
//range    0xFF000000 0xFFFFFFFF 1 ReadWrite

// CCS does not read correctly the values from 
// 0xFFFFFF00 to 0xFFFFFFFF from flash with access size 1-byte
// workaround added: read the last 256 bytes using 4-bytes access
range    0xFF000000 0xFFFFFEFF 1 ReadWrite
range    0xFFFFFF00 0xFFFFFFFF 4 ReadWrite
