<SETUP CpuVendor="Atmel" CpuChip="AT91M40800" FlashVendor="Fujitsu" FlashChip="MBM29LV160TE" RamAddress="0x2200000" RamSize="0x400000" FlashAddress="0x1000000" FlashSize="0x100000" CpuType="ARM7TDMI" CpuFamily="ARM" Register7="0x3" ManufacturersCode="0X04" DeviceID="0X22C4" INIFile="" FailMask="0x0" CpuEndian="Little" LoadFileLE="arm7.bin" LoadFileBE="arm7be.bin" Regcount="0x3c" Seccount="0x23" FlashWidth="0x80" FlashChipsPerSector="0x1">
    <Regcount Regcount="0x3c">
        <Sim Register="EBI_CSR0" Address="0XFFE00000" Value="0X0000203D" Default="0X0000203D" Width="32" />
        <Sim Register="EBI_CSR1" Address="0XFFE00004" Value="0X10000000" Default="0X10000000" Width="32" />
        <Sim Register="EBI_CSR2" Address="0XFFE00008" Value="0X20000000" Default="0X20000000" Width="32" />
        <Sim Register="EBI_CSR3" Address="0XFFE0000C" Value="0X30000000" Default="0X30000000" Width="32" />
        <Sim Register="EBI_CSR4" Address="0XFFE00010" Value="0X40000000" Default="0X40000000" Width="32" />
        <Sim Register="EBI_CSR5" Address="0XFFE00014" Value="0X50000000" Default="0X50000000" Width="32" />
        <Sim Register="EBI_CSR6" Address="0XFFE00018" Value="0X60000000" Default="0X60000000" Width="32" />
        <Sim Register="EBI_CSR7" Address="0XFFE0001C" Value="0X70000000" Default="0X70000000" Width="32" />
        <Sim Register="EBI_RCR" Address="0XFFE00020" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="EBI_MCR" Address="0XFFE00024" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="AIC_IECR" Address="0XFFFFF120" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="AIC_IDCR" Address="0XFFFFF124" Value="0XFFFFFFFF" Default="0XFFFFFFFF" Width="32" />
        <Sim Register="PIO_PER" Address="0XFFFF0000" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_PDR" Address="0XFFFF0004" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_OER" Address="0XFFFF0010" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_ODR" Address="0XFFFF0014" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_IFER" Address="0XFFFF0020" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_IFDR" Address="0XFFFF0024" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_SODR" Address="0XFFFF0030" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_CODR" Address="0XFFFF0034" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_IER" Address="0XFFFF0040" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="PIO_IDR" Address="0XFFFF0044" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US0_CR" Address="0XFFFD0000" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US0_MR" Address="0XFFFD0004" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US0_IER" Address="0XFFFD0008" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US0_IDR" Address="0XFFFD000C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US1_CR" Address="0XFFFC0000" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US1_MR" Address="0XFFFC0004" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US1_IER" Address="0XFFFC0008" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US1_IDR" Address="0XFFFC000C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="US1_IDR" Address="0XFFFC000C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_CCR" Address="0XFFFE0000" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_CMR" Address="0XFFFE0004" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_CV" Address="0XFFFE0010" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_RA" Address="0XFFFE0014" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_RB" Address="0XFFFE0018" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_RC" Address="0XFFFE001C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_IER" Address="0XFFFE0024" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC0_IDR" Address="0XFFFE0028" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_CCR" Address="0XFFFE0040" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_CMR" Address="0XFFFE0044" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_CV" Address="0XFFFE0050" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_RA" Address="0XFFFE0054" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_RB" Address="0XFFFE0058" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_RC" Address="0XFFFE005C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_IER" Address="0XFFFE0064" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC1_IDR" Address="0XFFFE0068" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_CCR" Address="0XFFFE0080" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_CMR" Address="0XFFFE0084" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_CV" Address="0XFFFE0090" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_RA" Address="0XFFFE0094" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_RB" Address="0XFFFE0098" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_RC" Address="0XFFFE009C" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_IER" Address="0XFFFE00A4" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC2_IDR" Address="0XFFFE00A8" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC_BCR" Address="0XFFFE00C0" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="TC_BMR" Address="0XFFFE00C4" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="WD_OMR" Address="0XFFFF8000" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="WD_CMR" Address="0XFFFF8004" Value="0X0" Default="0X0" Width="32" />
        <Sim Register="WD_CR" Address="0XFFFF8008" Value="0X0" Default="0X0" Width="32" />
    </Regcount>
    <Seccount Seccount="0x23">
        <Sector1 Sector="1" Size="65536" />
        <Sector32 Sector="32" Size="32768" />
        <Sector33 Sector="33" Size="8192" />
        <Sector35 Sector="35" Size="16384" />
    </Seccount>
    <CommandType name="FUJITSU:LV8/16">
        <Item DResetSequence="1" D8Reset1A="0X0" D8Reset1D="0XF0" D16Reset1A="0X0" D16Reset1D="0X00F0" DGetMCSequence="4" D8GetMC1A="0XAAA" D8GetMC1D="0XAA" D8GetMC2A="0X555" D8GetMC2D="0X55" D8GetMC3A="0XAAA" D8GetMC3D="0X90" D8GetMC4A="0X00" D8GetMC4D="READ" D16GetMC1A="0X555" D16GetMC1D="0XAAAA" D16GetMC2A="0X2AA" D16GetMC2D="0X5555" D16GetMC3A="0X555" D16GetMC3D="0X0090" D16GetMC4A="0X0000" D16GetMC4D="READ" DGetDIDSequence="4" D8GetDID1A="0XAAA" D8GetDID1D="0XAA" D8GetDID2A="0X555" D8GetDID2D="0X55" D8GetDID3A="0XAAA" D8GetDID3D="0X90" D8GetDID4A="0X01" D8GetDID4D="READ" D16GetDID1A="0X555" D16GetDID1D="0XAAAA" D16GetDID2A="0X2AA" D16GetDID2D="0X5555" D16GetDID3A="0X555" D16GetDID3D="0X0090" D16GetDID4A="0X01" D16GetDID4D="READ" DChipEraseSequence="6" D8ChipErase1A="0XAAA" D8ChipErase1D="0XAA" D8ChipErase2A="0X555" D8ChipErase2D="0X55" D8ChipErase3A="0XAAA" D8ChipErase3D="0X80" D8ChipErase4A="0XAAA" D8ChipErase4D="0XAA" D8ChipErase5A="0X555" D8ChipErase5D="0X55" D8ChipErase6A="0XAAA" D8ChipErase6D="0X10" D16ChipErase1A="0X555" D16ChipErase1D="0XAAAA" D16ChipErase2A="0X2AA" D16ChipErase2D="0X5555" D16ChipErase3A="0X555" D16ChipErase3D="0X0080" D16ChipErase4A="0X555" D16ChipErase4D="0XAAAA" D16ChipErase5A="0X2AA" D16ChipErase5D="0X5555" D16ChipErase6A="0X555" D16ChipErase6D="0X0010" DSectorEraseSequence="6" D8SectorErase1A="0XAAA" D8SectorErase1D="0XAA" D8SectorErase2A="0X555" D8SectorErase2D="0X55" D8SectorErase3A="0XAAA" D8SectorErase3D="0X80" D8SectorErase4A="0XAAA" D8SectorErase4D="0XAA" D8SectorErase5A="0X555" D8SectorErase5D="0X55" D8SectorErase6A="WRITE" D8SectorErase6D="0X30" D16SectorErase1A="0X555" D16SectorErase1D="0XAAAA" D16SectorErase2A="0X2AA" D16SectorErase2D="0X5555" D16SectorErase3A="0X555" D16SectorErase3D="0X0080" D16SectorErase4A="0X555" D16SectorErase4D="0XAAAA" D16SectorErase5A="0X2AA" D16SectorErase5D="0X5555" D16SectorErase6A="WRITE" D16SectorErase6D="0X0030" DProgramSequence="3" D8Program1A="0XAAA" D8Program1D="0XAA" D8Program2A="0X555" D8Program2D="0X55" D8Program3A="0XAAA" D8Program3D="0XA0" D16Program1A="0X555" D16Program1D="0XAAAA" D16Program2A="0X2AA" D16Program2D="0X5555" D16Program3A="0X555" D16Program3D="0X00A0" />
    </CommandType>
    <Param FlashStart="0x1000000" FileStart="0x0" FileEnd="0x0" />
</SETUP>
