<SETUP CpuVendor="Atmel" CpuChip="AT91M40400" FlashVendor="Atmel" FlashChip="AT29LV1024" ManufacturersCode="0X1F" DeviceID="0X26" RamAddress="0x00300000" FlashAddress="0x00000000" CpuType="ARM7TDMI" CpuFamily="ARM" Register7="5" LoadFileLE="arm7.bin" LoadFileBE="arm7be.bin" Regcount="60" Seccount="512" FlashWidth="16" FlashChipsPerSector="1">
    <Regcount Regcount="60">
        <Sim name="Sim1" Register="EBI_CSR0" Address="0XFFE00000" Value="0X0000203D" Default="0X0000203D" Width="32" ReadWrite="0" />
        <Sim name="Sim2" Register="EBI_CSR1" Address="0XFFE00004" Value="0X10000000" Default="0X10000000" Width="32" ReadWrite="0" />
        <Sim name="Sim3" Register="EBI_CSR2" Address="0XFFE00008" Value="0X20000000" Default="0X20000000" Width="32" ReadWrite="0" />
        <Sim name="Sim4" Register="EBI_CSR3" Address="0XFFE0000C" Value="0X30000000" Default="0X30000000" Width="32" ReadWrite="0" />
        <Sim name="Sim5" Register="EBI_CSR4" Address="0XFFE00010" Value="0X40000000" Default="0X40000000" Width="32" ReadWrite="0" />
        <Sim name="Sim6" Register="EBI_CSR5" Address="0XFFE00014" Value="0X50000000" Default="0X50000000" Width="32" ReadWrite="0" />
        <Sim name="Sim7" Register="EBI_CSR6" Address="0XFFE00018" Value="0X60000000" Default="0X60000000" Width="32" ReadWrite="0" />
        <Sim name="Sim8" Register="EBI_CSR7" Address="0XFFE0001C" Value="0X70000000" Default="0X70000000" Width="32" ReadWrite="0" />
        <Sim name="Sim9" Register="EBI_RCR" Address="0XFFE00020" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim10" Register="EBI_MCR" Address="0XFFE00024" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim11" Register="AIC_IECR" Address="0XFFFFF120" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim12" Register="AIC_IDCR" Address="0XFFFFF124" Value="0XFFFFFFFF" Default="0XFFFFFFFF" Width="32" ReadWrite="0" />
        <Sim name="Sim13" Register="PIO_PER" Address="0XFFFF0000" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim14" Register="PIO_PDR" Address="0XFFFF0004" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim15" Register="PIO_OER" Address="0XFFFF0010" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim16" Register="PIO_ODR" Address="0XFFFF0014" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim17" Register="PIO_IFER" Address="0XFFFF0020" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim18" Register="PIO_IFDR" Address="0XFFFF0024" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim19" Register="PIO_SODR" Address="0XFFFF0030" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim20" Register="PIO_CODR" Address="0XFFFF0034" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim21" Register="PIO_IER" Address="0XFFFF0040" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim22" Register="PIO_IDR" Address="0XFFFF0044" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim23" Register="US0_CR" Address="0XFFFD0000" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim24" Register="US0_MR" Address="0XFFFD0004" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim25" Register="US0_IER" Address="0XFFFD0008" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim26" Register="US0_IDR" Address="0XFFFD000C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim27" Register="US1_CR" Address="0XFFFC0000" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim28" Register="US1_MR" Address="0XFFFC0004" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim29" Register="US1_IER" Address="0XFFFC0008" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim30" Register="US1_IDR" Address="0XFFFC000C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim31" Register="US1_IDR" Address="0XFFFC000C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim32" Register="TC0_CCR" Address="0XFFFE0000" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim33" Register="TC0_CMR" Address="0XFFFE0004" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim34" Register="TC0_CV" Address="0XFFFE0010" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim35" Register="TC0_RA" Address="0XFFFE0014" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim36" Register="TC0_RB" Address="0XFFFE0018" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim37" Register="TC0_RC" Address="0XFFFE001C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim38" Register="TC0_IER" Address="0XFFFE0024" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim39" Register="TC0_IDR" Address="0XFFFE0028" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim40" Register="TC1_CCR" Address="0XFFFE0040" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim41" Register="TC1_CMR" Address="0XFFFE0044" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim42" Register="TC1_CV" Address="0XFFFE0050" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim43" Register="TC1_RA" Address="0XFFFE0054" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim44" Register="TC1_RB" Address="0XFFFE0058" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim45" Register="TC1_RC" Address="0XFFFE005C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim46" Register="TC1_IER" Address="0XFFFE0064" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim47" Register="TC1_IDR" Address="0XFFFE0068" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim48" Register="TC2_CCR" Address="0XFFFE0080" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim49" Register="TC2_CMR" Address="0XFFFE0084" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim50" Register="TC2_CV" Address="0XFFFE0090" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim51" Register="TC2_RA" Address="0XFFFE0094" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim52" Register="TC2_RB" Address="0XFFFE0098" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim53" Register="TC2_RC" Address="0XFFFE009C" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim54" Register="TC2_IER" Address="0XFFFE00A4" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim55" Register="TC2_IDR" Address="0XFFFE00A8" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim56" Register="TC_BCR" Address="0XFFFE00C0" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim57" Register="TC_BMR" Address="0XFFFE00C4" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim58" Register="WD_OMR" Address="0XFFFF8000" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim59" Register="WD_CMR" Address="0XFFFF8004" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
        <Sim name="Sim60" Register="WD_CR" Address="0XFFFF8008" Value="0X0" Default="0X0" Width="32" ReadWrite="0" />
    </Regcount>
    <Seccount Seccount="512">
        <Sector1 Sector="1" Size="256" />
    </Seccount>
    <CommandType name="ATMEL:C16">
        <Item DResetSequence="6" D16Reset1A="0X5555" D16Reset1D="0XAAAA" D16Reset2A="0X2AAA" D16Reset2D="0X5555" D16Reset3A="0X5555" D16Reset3D="0X8080" D16Reset4A="0X5555" D16Reset4D="0XAAAA" D16Reset5A="0X2AAA" D16Reset5D="0X5555" D16Reset6A="0X5555" D16Reset6D="0X2020" DGetMCSequence="4" D16GetMC1A="0X5555" D16GetMC1D="0XAAAA" D16GetMC2A="0X2AAA" D16GetMC2D="0X5555" D16GetMC3A="0X5555" D16GetMC3D="0X9090" D16GetMC4A="0X00" D16GetMC4D="READ" DGetDIDSequence="4" D16GetDID1A="0X5555" D16GetDID1D="0XAAAA" D16GetDID2A="0X2AAA" D16GetDID2D="0X5555" D16GetDID3A="0X5555" D16GetDID3D="0X9090" D16GetDID4A="0X01" D16GetDID4D="READ" DReadSequence="3" D16Read1A="0X5555" D16Read1D="0XAAAA" D16Read2A="0X2AAA" D16Read2D="0X5555" D16Read3A="0X5555" D16Read3D="0XF0F0" DChipEraseSequence="0" D16ChipErase1A="0X5555" D16ChipErase1D="0XAAAA" D16ChipErase2A="0X2AAA" D16ChipErase2D="0X5555" D16ChipErase3A="0X5555" D16ChipErase3D="0X8080" D16ChipErase4A="0X5555" D16ChipErase4D="0XAAAA" D16ChipErase5A="0X2AAA" D16ChipErase5D="0X5555" D16ChipErase6A="0X5555" D16ChipErase6D="0X1010" DSectorEraseWaitTime="3" DSectorEraseSequence="3" D16SectorErase1A="0X5555" D16SectorErase1D="0XAAAA" D16SectorErase2A="0X2AAA" D16SectorErase2D="0X5555" D16SectorErase3A="0X5555" D16SectorErase3D="0XA0A0" DProgramSequence="3" D16Program1A="0X5555" D16Program1D="0XAAAA" D16Program2A="0X2AAA" D16Program2D="0X5555" D16Program3A="0X5555" D16Program3D="0XA0A0" />
    </CommandType>
</SETUP>
