<SETUP CpuVendor="Atmel" CpuChip="AT91M40800" FlashVendor="Atmel" FlashChip="AT49BV161T" RamAddress="0x2000000" RamSize="0x400000" FlashAddress="0x1000000" FlashSize="0x100000" CpuType="ARM7TDMI" CpuFamily="ARM" Register7="0x3" ManufacturersCode="0X1F" DeviceID="0X00C2" INIFile="" FailMask="0x0" CpuEndian="Little" LoadFileLE="arm7.bin" LoadFileBE="arm7be.bin" Regcount="0xa" Seccount="0x27" FlashWidth="0x10" FlashChipsPerSector="0x1">
    <Regcount Regcount="0xa">
        <Sim Register="0xffe00000" Address="0xffe00000" Value="0x01002529" Default="0x0" Width="32" />
        <Sim Register="0xffe00004" Address="0xffe00004" Value="0x022028a1" Default="0x0" Width="32" />
        <Sim Register="0xffe00008" Address="0xffe00008" Value="0x03002529" Default="0x0" Width="32" />
        <Sim Register="0xffe0000c" Address="0xffe0000c" Value="0x40000000" Default="0x0" Width="32" />
        <Sim Register="0xffe00010" Address="0xffe00010" Value="0x02402021" Default="0x0" Width="32" />
        <Sim Register="0xffe00014" Address="0xffe00014" Value="0x02502021" Default="0x0" Width="32" />
        <Sim Register="0xffe00018" Address="0xffe00018" Value="0x60000000" Default="0x0" Width="32" />
        <Sim Register="0xffe0001c" Address="0xffe0001c" Value="0x70000000" Default="0x0" Width="32" />
        <Sim Register="0xffe00020" Address="0xffe00020" Value="0x00000001" Default="0x0" Width="32" />
        <Sim Register="0xffe00024" Address="0xffe00024" Value="0x00000006" Default="0x0" Width="32" />
    </Regcount>
    <Seccount Seccount="0x27">
        <Sector1 Sector="1" Size="65536" />
        <Sector32 Sector="32" Size="8192" />
    </Seccount>
    <CommandType name="ATMEL:49">
        <type name="ATMEL:49">
            <BUS width="8">
                <reset>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0XF0" />
                </reset>
                <MC>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X90" />
                    <item addr="0X00" data="READ" />
                </MC>
                <DID>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X90" />
                    <item addr="0X01" data="READ" />
                </DID>
                <GetProtect>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X90" />
                    <item addr="0X02" data="READ" />
                    <item addr="0X0" data="0XF0" />
                </GetProtect>
                <SectorProtect>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X80" />
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X0" data="0X40" />
                </SectorProtect>
                <ChipErase>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X80" />
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0X2AAA" data="0X55" />
                    <item addr="0X5555" data="0X10" />
                </ChipErase>
                <SectorErase>
                    <item addr="0X5555" data="0XAA" />
                    <item addr="0x2AAA" data="0x55" />
                    <item addr="0x5555" data="0x80" />
                    <item addr="0x5555" data="AA" />
                    <item addr="0x2AAA" data="0x55" />
                    <item addr="WRITE" data="0x30" />
                </SectorErase>
                <Program>
                    <item addr="0x5555" data="0xAA" />
                    <item addr="0x2AAA" data="0x55" />
                    <item addr="0x5555" data="0xA0" />
                </Program>
            </BUS>
            <BUS width="16">
                <reset>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0XF0F0" />
                </reset>
                <MC>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X9090" />
                    <item addr="0X0000" data="READ" />
                </MC>
                <DID>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X9090" />
                    <item addr="0X0101" data="READ" />
                </DID>
                <GetProtect>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X9090" />
                    <item addr="0X0002" data="READ" />
                    <item addr="0X0" data="0XF0F0" />
                </GetProtect>
                <SectorProtect>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X8080" />
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X0" data="0X4040" />
                </SectorProtect>
                <ChipErase>
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X8080" />
                    <item addr="0X5555" data="0XAAAA" />
                    <item addr="0X2AAA" data="0X5555" />
                    <item addr="0X5555" data="0X1010" />
                </ChipErase>
                <SectorErase>
                    <item addr="0x5555" data="0xAAAA" />
                    <item addr="0x2AAA" data="0x5555" />
                    <item addr="0x5555" data="0x8080" />
                    <item addr="0x5555" data="0xAAAA" />
                    <item addr="0x2AAA" data="0x5555" />
                    <item addr="WRITE" data="0x3030" />
                </SectorErase>
                <Program>
                    <item addr="0x5555" data="0xAAAA" />
                    <item addr="0x2AAA" data="0x5555" />
                    <item addr="0x5555" data="0xA0A0" />
                </Program>
            </BUS>
        </type>
    </CommandType>
    <Param FlashStart="0x1000000" FileStart="0x0" FileEnd="0x0" />
</SETUP>
