CodeWarrior USB Device Driver Manual Installation:
--------------------------------------------------

Supported Devices:

  CodeWarrior USB TAP
  CodeWarrior HTI

Supported Operating Systems:

  Windows NT 4
  Windows 2000
  Windows XP

Driver Type:

  Jungo WinDriver Version 7.0

Installation Instructions:

  Please note that the following procedures assume that the user has 
  the Administrator privileges.

  1.  Launch a Windows command shell and change the driver directory:

      Start->Programs->Accessories->Command Prompt
      C:\Profiles\Username> cd "\Program Files\Freescale\CodeWarrior"
      C:\Program Files\Freescale\CodeWarrior> cd "ccs\drivers\usb"

  2.  Unplug all USB TAPs and USB HTIs from your machine

  3.  Install the driver with the setup command:

      C:\Program Files\...\usb> setup

  3.  Plug in USB TAPs and USB HTIs

  4.  The Found New Hardware Wizard will run, browse to usbtap.inf which is
      is located in the ccs/drivers/usb folder
