$variable   [=value]
ACcess      [-B|-Hw|-W]
ALias       [original_name new_name]
Assemble    [adr]
Breakpoint  [adr]
BYte        adr datum1 [..datum32]
CLear       {All|address|HW0|HW1}
COMpare     adr1 {adr2|Length length} adr3 [-B|-Hw|-W]
Copy        adr1 {adr2|Length length} adr3 [-B|-Hw|-W]
CReate      #symbol adr
DElete      #symbol|$variable|All
Disassemble [adr1 [adr2|Length length]]
Fill        adr1 {adr2|Length length} {"string"|data.. [-B|-Hw|-W]}
Go          [[Run][From adr1]|[From adr1][Till adr2]|[Monitor timer]]
HAlt
Help        [command]
Include     filename
INPort      port [len] [-B|-Hw|-W] [filename] [COUNT count [ctrladdr1 ctrldata [-B|-Hw|-W] [PRE|POST] [ctrladdr1 ctrldata [-B|-Hw|-W] [PRE|POST] ...] ] ]
			(Not avaliable in simulator version.)
Jump        adr
LOad        filename [Symbols|NOSymbols] [Code|NOCode] [Warn|NOWarn] [S-R|BIN addr|DIS addr|DISA|DISC addr|DISAC|EXEC]
LOG         {filename [Command] [Append]}|{On|OFf|CLear}
LONg        adr data1 [..data32]
Memory      adr1 [adr2|Length length] [-B|-Hw|-W]
Outport     port [INC] {data...|File filename [Offset offset]} [Length length] [-B|-Hw|-W] [Count count [ctrladdr1 ctrldata [-B|-Hw|-W] [PRE|POST] [ctrladdr1 ctrldata [-B|-Hw|-W] [PRE|POST] ...] ] ]
			(Not avaliable in simulator version.)
QUEry       #symbol|hex_adr
Register    [{reg_id} [data]]
RESet       [adr]
RESTart
SAvedisasm  adr1 {adr2|Length length} filename
SEarch	    adr1 {adr2|Length length} {[Insensitive] "string"|data..}
SRecall     filename
SSave       filename
Step        [[Over] [count] | FOrever | Till {Ret|Call} | Till {@reg|adr} Is value ]
SYmbol      [Global|Module|#module|Lines]
TEst        adr1 {adr2|Length length}[Mem|DAta|ADdr][-B|-Hw|-W]
			(Not avaliable in simulator version.)
Upload      adr1 {adr2|Length length} filename [S-R|BIN|DIS|DISA|DISC|DISAC]
WAtch       "C-Expression"
Watchpoint  [ADdr addr][AMask mask][DAta data][DMask mask][-B|-Hw|-W][Fetch|Access][Read|Write][HW0|HW1]
WOrd        adr data1 [..data32]


