Static Call Graph - [.\Obj\RTX_Session5.axf]

# Static Call Graph for image .\Obj\RTX_Session5.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 713]: Last Updated: Tue Sep 13 13:42:39 2011

### Maximum Stack Usage = 524 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

ADC_Calc_Task ⇒ ADC_Average_Samples ⇒ arm_dot_prod_f32 ⇒ __aeabi_fadd ⇒ _float_epilogue

### Functions with no stack information

- SysTick_Handler

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- Default_Handler ⇒ Default_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - ADC_Calc_Task from rt_adc.o(.text) referenced from main.o(.text)
  - ADC_Sample_Task from rt_adc.o(.text) referenced from main.o(.text)
  - BusFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - Button_Task from rt_gpio.o(.text) referenced from main.o(.text)
  - CAN1_RX0_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - Default_Handler from startup_stm32f10x_cl.o(.text) referenced 7 times from startup_stm32f10x_cl.o(RESET)
  - ETH_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI0_IRQHandler from hal_gpio.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - HardFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - LED_Task from rt_gpio.o(.text) referenced from main.o(.text)
  - MemManage_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - NMI_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - PendSV_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - Reset_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SVC_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - SysTick_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - TAMPER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UART_Task from rt_serial.o(.text) referenced from main.o(.text)
  - USART1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_cl.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - fputc from retarget.o(.text) referenced from printfa.o(i.__0printf)
  - init from main.o(.text) referenced from main.o(.text)
  - main from main.o(.text) referenced from entry7.o(.ARM.Collect$$$$00000007)
  - os_idle_demon from rtx_conf_cm.o(.text) referenced from rt_task.o(i.rt_sys_init)
  - rt_alloc_box from rt_membox.o(i.rt_alloc_box) referenced from hal_cm3.o(.emb_text)
  - rt_dly_wait from rt_time.o(i.rt_dly_wait) referenced 2 times from rt_adc.o(.text)
  - rt_evt_clr from rt_event.o(i.rt_evt_clr) referenced from rt_gpio.o(.text)
  - rt_evt_get from rt_event.o(i.rt_evt_get) referenced from rt_adc.o(.text)
  - rt_evt_set from rt_event.o(i.rt_evt_set) referenced from rt_adc.o(.text)
  - rt_evt_wait from rt_event.o(i.rt_evt_wait) referenced 2 times from rt_adc.o(.text)
  - rt_free_box from rt_membox.o(i.rt_free_box) referenced from hal_cm3.o(.emb_text)
  - rt_mbx_init from rt_mailbox.o(i.rt_mbx_init) referenced from rt_serial.o(.text)
  - rt_mbx_send from rt_mailbox.o(i.rt_mbx_send) referenced 2 times from rt_adc.o(.text)
  - rt_mbx_wait from rt_mailbox.o(i.rt_mbx_wait) referenced from rt_serial.o(.text)
  - rt_sys_init from rt_task.o(i.rt_sys_init) referenced from main.o(.text)
  - rt_tsk_create from rt_task.o(i.rt_tsk_create) referenced from main.o(.text)
  - rt_tsk_delete from rt_task.o(i.rt_tsk_delete) referenced from main.o(.text)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  rt_set_PSP (Thumb, 6 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> rt_sys_init

  os_set_env (Thumb, 26 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> main

  _alloc_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> Button_Task
  - >> ADC_Calc_Task

  _free_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> UART_Task

  SVC_Handler (Thumb, 132 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Calls]

  - >> rt_stk_check
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  PendSV_Handler (Thumb, 0 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  Sys_Handler (Thumb, 84 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)
  [Calls]

  - >> rt_systick
  - >> rt_stk_check
  - >> rt_pop_req

  SysTick_Handler (Thumb, 0 bytes, Stack size unknown bytes, hal_cm3.o(.emb_text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SystemInit (Thumb, 456 bytes, Stack size 40 bytes, system_stm32f10x_cl.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = SystemInit ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_d2uiz
  [Called By]
  - >> InitHAL

  fputc (Thumb, 14 bytes, Stack size 16 bytes, retarget.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> sendchar
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  fgetc (Thumb, 10 bytes, Stack size 8 bytes, retarget.o(.text), UNUSED)
  [Calls]

  - >> getkey

  ferror (Thumb, 8 bytes, Stack size 0 bytes, retarget.o(.text), UNUSED)

  _ttywrch (Thumb, 12 bytes, Stack size 8 bytes, retarget.o(.text), UNUSED)
  [Calls]

  - >> sendchar

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, retarget.o(.text), UNUSED)

  os_idle_demon (Thumb, 6 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Address Reference Count : 1]

  - rt_task.o(i.rt_sys_init)

  os_tmr_call (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text), UNUSED)
  [Called By]

  - >> rt_tmr_tick

  os_error (Thumb, 4 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_mbx_psh
  - >> rt_psq_enq
  - >> rt_stk_check

  rt_init_robin (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_sys_init

  rt_chk_robin (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text), UNUSED)
  [Called By]

  - >> rt_systick

  init (Thumb, 108 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = init ⇒ _init_box
  [Calls]
  - >> _init_box
  [Address Reference Count : 1]
  - main.o(.text)

  main (Thumb, 40 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = main ⇒ InitHAL ⇒ SystemInit ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> os_set_env
  - >> InitSerial
  - >> InitHAL
  - >> InitGPIO
  - >> InitADC
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  ADC_Sample_Task (Thumb, 108 bytes, Stack size 0 bytes, rt_adc.o(.text))
  [Calls]

  - >> GetValADC
  [Address Reference Count : 1]
  - main.o(.text)

  ADC_Average_Samples (Thumb, 244 bytes, Stack size 440 bytes, rt_adc.o(.text))
  [Stack]

  - Max Depth = 524
  - Call Chain = ADC_Average_Samples ⇒ arm_dot_prod_f32 ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> arm_sub_f32
  - >> arm_mult_f32
  - >> arm_fill_f32
  - >> arm_dot_prod_f32
  - >> arm_copy_f32
  - >> __aeabi_ui2d
  - >> __aeabi_i2f
  - >> __aeabi_fmul
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> ADC_Calc_Task

  ADC_Calc_Task (Thumb, 84 bytes, Stack size 0 bytes, rt_adc.o(.text))
  [Stack]

  - Max Depth = 524
  - Call Chain = ADC_Calc_Task ⇒ ADC_Average_Samples ⇒ arm_dot_prod_f32 ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _alloc_box
  - >> __aeabi_f2d
  - >> ADC_Average_Samples
  - >> __2sprintf
  [Address Reference Count : 1]
  - main.o(.text)

  Button_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, rt_gpio.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Button_IRQHandler ⇒ isr_evt_set ⇒ rt_psq_enq
  [Calls]
  - >> isr_evt_set
  [Called By]
  - >> EXTI0_IRQHandler

  LED_Task (Thumb, 32 bytes, Stack size 0 bytes, rt_gpio.o(.text))
  [Calls]

  - >> LED_On
  - >> LED_Off
  [Address Reference Count : 1]
  - main.o(.text)

  Button_Task (Thumb, 78 bytes, Stack size 0 bytes, rt_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Button_Task ⇒ __2sprintf
  [Calls]
  - >> EnableButtonIRQ
  - >> _alloc_box
  - >> __2sprintf
  [Address Reference Count : 1]
  - main.o(.text)

  UART_Task (Thumb, 44 bytes, Stack size 8 bytes, rt_serial.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_Task ⇒ __2printf
  [Calls]
  - >> _free_box
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(.text)

  InitADC (Thumb, 138 bytes, Stack size 0 bytes, hal_adc.o(.text))
  [Called By]

  - >> main

  GetValADC (Thumb, 8 bytes, Stack size 0 bytes, hal_adc.o(.text))
  [Called By]

  - >> ADC_Sample_Task

  InitGPIO (Thumb, 66 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> main

  EnableButtonIRQ (Thumb, 32 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> Button_Task

  DisableButtonIRQ (Thumb, 26 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> EXTI0_IRQHandler

  EXTI0_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, hal_gpio.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EXTI0_IRQHandler ⇒ Button_IRQHandler ⇒ isr_evt_set ⇒ rt_psq_enq
  [Calls]
  - >> DisableButtonIRQ
  - >> Button_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  LED_On (Thumb, 12 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> LED_Task

  LED_Off (Thumb, 12 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> LED_Task

  LED_Toggle (Thumb, 20 bytes, Stack size 0 bytes, hal_gpio.o(.text), UNUSED)

  InitHAL (Thumb, 8 bytes, Stack size 8 bytes, hal.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = InitHAL ⇒ SystemInit ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> SystemInit
  [Called By]
  - >> main

  InitSerial (Thumb, 116 bytes, Stack size 0 bytes, hal_serial.o(.text))
  [Called By]

  - >> main

  sendchar (Thumb, 56 bytes, Stack size 0 bytes, hal_serial.o(.text))
  [Called By]

  - >> _ttywrch
  - >> fputc

  getkey (Thumb, 22 bytes, Stack size 0 bytes, hal_serial.o(.text), UNUSED)
  [Called By]

  - >> fgetc

  arm_dot_prod_f32 (Thumb, 414 bytes, Stack size 64 bytes, arm_dot_prod_f32.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = arm_dot_prod_f32 ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  - >> __aeabi_fmul
  [Called By]
  - >> ADC_Average_Samples

  arm_mult_f32 (Thumb, 284 bytes, Stack size 56 bytes, arm_mult_f32.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = arm_mult_f32 ⇒ __aeabi_fmul
  [Calls]
  - >> __aeabi_fmul
  [Called By]
  - >> ADC_Average_Samples

  arm_sub_f32 (Thumb, 284 bytes, Stack size 56 bytes, arm_sub_f32.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = arm_sub_f32 ⇒ __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fsub
  [Called By]
  - >> ADC_Average_Samples

  arm_copy_f32 (Thumb, 170 bytes, Stack size 12 bytes, arm_copy_f32.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = arm_copy_f32
  [Called By]
  - >> ADC_Average_Samples

  arm_fill_f32 (Thumb, 130 bytes, Stack size 4 bytes, arm_fill_f32.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = arm_fill_f32
  [Called By]
  - >> ADC_Average_Samples

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> __aeabi_fsub
  - >> arm_dot_prod_f32
  - >> __aeabi_frsub

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> arm_sub_f32

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fadd

  __aeabi_fmul (Thumb, 108 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> arm_mult_f32
  - >> arm_dot_prod_f32
  - >> ADC_Average_Samples

  __aeabi_dmul (Thumb, 224 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> SystemInit
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> ADC_Average_Samples
  - >> _fp_digits

  __aeabi_i2f (Thumb, 18 bytes, Stack size 0 bytes, fflti.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_i2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> ADC_Average_Samples

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> SystemInit

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> ADC_Average_Samples

  __aeabi_d2uiz (Thumb, 46 bytes, Stack size 0 bytes, dfixui.o(.text))
  [Calls]

  - >> __aeabi_llsr
  [Called By]
  - >> SystemInit

  __aeabi_f2d (Thumb, 44 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> ADC_Calc_Task

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Calls]
  - >> _float_round
  [Called By]
  - >> ADC_Average_Samples

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fadd
  - >> __aeabi_d2f

  _float_epilogue (Thumb, 90 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_fadd
  - >> __aeabi_i2f

  _double_round (Thumb, 26 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> _double_epilogue
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 168 bytes, Stack size 48 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> _double_round
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_dadd (Thumb, 318 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  - >> _double_epilogue
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 38 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> UART_Task

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> Button_Task
  - >> ADC_Calc_Task

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  _init_box (Thumb, 70 bytes, Stack size 8 bytes, rt_membox.o(i._init_box))
  [Stack]

  - Max Depth = 8
  - Call Chain = _init_box
  [Called By]
  - >> rt_sys_init
  - >> init

  dbg_init (Thumb, 36 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_init))
  [Called By]

  - >> rt_sys_init

  dbg_task_notify (Thumb, 32 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_task_notify))
  [Called By]

  - >> rt_tsk_delete
  - >> rt_tsk_create

  dbg_task_switch (Thumb, 16 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_task_switch))
  [Called By]

  - >> rt_switch_req

  isr_evt_set (Thumb, 34 bytes, Stack size 8 bytes, rt_event.o(i.isr_evt_set))
  [Stack]

  - Max Depth = 24
  - Call Chain = isr_evt_set ⇒ rt_psq_enq
  [Calls]
  - >> rt_psq_enq
  - >> rt_psh_req
  [Called By]
  - >> Button_IRQHandler

  rt_alloc_box (Thumb, 28 bytes, Stack size 0 bytes, rt_membox.o(i.rt_alloc_box))
  [Called By]

  - >> rt_init_context
  - >> rt_tsk_create
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_block (Thumb, 48 bytes, Stack size 16 bytes, rt_task.o(i.rt_block))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_put_dly
  - >> rt_get_first
  - >> rt_switch_req
  [Called By]
  - >> rt_mbx_wait
  - >> rt_mbx_send
  - >> rt_evt_wait
  - >> rt_dly_wait

  rt_dec_dly (Thumb, 106 bytes, Stack size 16 bytes, rt_list.o(i.rt_dec_dly), UNUSED)
  [Calls]

  - >> rt_put_prio
  [Called By]
  - >> rt_systick

  rt_dispatch (Thumb, 60 bytes, Stack size 16 bytes, rt_task.o(i.rt_dispatch))
  [Stack]

  - Max Depth = 28
  - Call Chain = rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_put_rdy_first
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_switch_req
  [Called By]
  - >> rt_mbx_wait
  - >> rt_mbx_send
  - >> rt_evt_set
  - >> rt_tsk_delete
  - >> rt_tsk_create

  rt_dly_wait (Thumb, 6 bytes, Stack size 0 bytes, rt_time.o(i.rt_dly_wait))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_dly_wait ⇒ rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_block
  [Address Reference Count : 2]
  - rt_adc.o(.text)
  - rt_gpio.o(.text)

  rt_evt_clr (Thumb, 22 bytes, Stack size 0 bytes, rt_event.o(i.rt_evt_clr))
  [Address Reference Count : 1]

  - rt_gpio.o(.text)

  rt_evt_get (Thumb, 8 bytes, Stack size 0 bytes, rt_event.o(i.rt_evt_get))
  [Address Reference Count : 1]

  - rt_adc.o(.text)

  rt_evt_psh (Thumb, 72 bytes, Stack size 8 bytes, rt_event.o(i.rt_evt_psh), UNUSED)
  [Calls]

  - >> rt_rmv_dly
  - >> rt_put_prio
  [Called By]
  - >> rt_pop_req

  rt_evt_set (Thumb, 90 bytes, Stack size 16 bytes, rt_event.o(i.rt_evt_set))
  [Stack]

  - Max Depth = 44
  - Call Chain = rt_evt_set ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_dispatch
  [Address Reference Count : 1]
  - rt_adc.o(.text)

  rt_evt_wait (Thumb, 58 bytes, Stack size 16 bytes, rt_event.o(i.rt_evt_wait))
  [Stack]

  - Max Depth = 40
  - Call Chain = rt_evt_wait ⇒ rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_block
  [Address Reference Count : 2]
  - rt_adc.o(.text)
  - rt_gpio.o(.text)

  rt_free_box (Thumb, 32 bytes, Stack size 0 bytes, rt_membox.o(i.rt_free_box))
  [Called By]

  - >> rt_tsk_delete
  - >> rt_tmr_tick
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_get_first (Thumb, 40 bytes, Stack size 0 bytes, rt_list.o(i.rt_get_first))
  [Called By]

  - >> rt_mbx_psh
  - >> rt_dispatch
  - >> rt_block
  - >> rt_mbx_wait
  - >> rt_mbx_send
  - >> rt_sem_psh
  - >> rt_systick
  - >> rt_pop_req

  rt_init_stack (Thumb, 70 bytes, Stack size 8 bytes, hal_cm3.o(i.rt_init_stack))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_init_stack
  [Called By]
  - >> rt_init_context

  rt_mbx_init (Thumb, 24 bytes, Stack size 0 bytes, rt_mailbox.o(i.rt_mbx_init))
  [Address Reference Count : 1]

  - rt_serial.o(.text)

  rt_mbx_psh (Thumb, 188 bytes, Stack size 24 bytes, rt_mailbox.o(i.rt_mbx_psh), UNUSED)
  [Calls]

  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  - >> os_error
  [Called By]
  - >> rt_pop_req

  rt_mbx_send (Thumb, 158 bytes, Stack size 24 bytes, rt_mailbox.o(i.rt_mbx_send))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_mbx_send ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  - >> rt_block
  [Address Reference Count : 2]
  - rt_adc.o(.text)
  - rt_gpio.o(.text)

  rt_mbx_wait (Thumb, 174 bytes, Stack size 24 bytes, rt_mailbox.o(i.rt_mbx_wait))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_mbx_wait ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  - >> rt_block
  [Address Reference Count : 1]
  - rt_serial.o(.text)

  rt_pop_req (Thumb, 114 bytes, Stack size 16 bytes, rt_system.o(i.rt_pop_req), UNUSED)
  [Calls]

  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_put_rdy_first
  - >> rt_get_first
  - >> rt_switch_req
  - >> rt_sem_psh
  [Called By]
  - >> Sys_Handler

  rt_psh_req (Thumb, 22 bytes, Stack size 0 bytes, rt_system.o(i.rt_psh_req))
  [Called By]

  - >> isr_evt_set

  rt_psq_enq (Thumb, 82 bytes, Stack size 16 bytes, rt_list.o(i.rt_psq_enq))
  [Stack]

  - Max Depth = 16
  - Call Chain = rt_psq_enq
  [Calls]
  - >> os_error
  [Called By]
  - >> isr_evt_set

  rt_put_dly (Thumb, 68 bytes, Stack size 8 bytes, rt_list.o(i.rt_put_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_put_dly
  [Called By]
  - >> rt_block

  rt_put_prio (Thumb, 54 bytes, Stack size 12 bytes, rt_list.o(i.rt_put_prio))
  [Stack]

  - Max Depth = 12
  - Call Chain = rt_put_prio
  [Called By]
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_dispatch
  - >> rt_mbx_wait
  - >> rt_mbx_send
  - >> rt_sem_psh
  - >> rt_dec_dly

  rt_put_rdy_first (Thumb, 14 bytes, Stack size 0 bytes, rt_list.o(i.rt_put_rdy_first))
  [Called By]

  - >> rt_dispatch
  - >> rt_systick
  - >> rt_pop_req

  rt_rmv_dly (Thumb, 40 bytes, Stack size 8 bytes, rt_list.o(i.rt_rmv_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_rmv_dly
  [Called By]
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_mbx_wait
  - >> rt_mbx_send
  - >> rt_evt_set
  - >> rt_tsk_delete
  - >> rt_sem_psh

  rt_rmv_list (Thumb, 44 bytes, Stack size 0 bytes, rt_list.o(i.rt_rmv_list))
  [Called By]

  - >> rt_tsk_delete

  rt_sem_psh (Thumb, 46 bytes, Stack size 8 bytes, rt_semaphore.o(i.rt_sem_psh), UNUSED)
  [Calls]

  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  [Called By]
  - >> rt_pop_req

  rt_stk_check (Thumb, 28 bytes, Stack size 0 bytes, rt_system.o(i.rt_stk_check))
  [Calls]

  - >> os_error
  [Called By]
  - >> Sys_Handler
  - >> SVC_Handler

  rt_switch_req (Thumb, 30 bytes, Stack size 0 bytes, rt_task.o(i.rt_switch_req))
  [Calls]

  - >> dbg_task_switch
  [Called By]
  - >> rt_dispatch
  - >> rt_block
  - >> rt_systick
  - >> rt_pop_req

  rt_sys_init (Thumb, 244 bytes, Stack size 24 bytes, rt_task.o(i.rt_sys_init))
  [Stack]

  - Max Depth = 76
  - Call Chain = rt_sys_init ⇒ rt_tsk_create ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_set_PSP
  - >> dbg_init
  - >> rt_init_context
  - >> rt_tsk_create
  - >> _init_box
  - >> rt_init_robin
  [Address Reference Count : 1]
  - main.o(.text)

  rt_systick (Thumb, 48 bytes, Stack size 8 bytes, rt_system.o(i.rt_systick), UNUSED)
  [Calls]

  - >> rt_put_rdy_first
  - >> rt_get_first
  - >> rt_switch_req
  - >> rt_chk_robin
  - >> rt_tmr_tick
  - >> rt_dec_dly
  [Called By]
  - >> Sys_Handler

  rt_tmr_tick (Thumb, 56 bytes, Stack size 16 bytes, rt_timer.o(i.rt_tmr_tick), UNUSED)
  [Calls]

  - >> rt_free_box
  - >> os_tmr_call
  [Called By]
  - >> rt_systick

  rt_tsk_create (Thumb, 122 bytes, Stack size 24 bytes, rt_task.o(i.rt_tsk_create))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_tsk_create ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_alloc_box
  - >> dbg_task_notify
  - >> rt_dispatch
  - >> rt_init_context
  [Called By]
  - >> rt_sys_init
  [Address Reference Count : 1]
  - main.o(.text)

  rt_tsk_delete (Thumb, 146 bytes, Stack size 24 bytes, rt_task.o(i.rt_tsk_delete))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_tsk_delete ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_list
  - >> rt_rmv_dly
  - >> rt_free_box
  - >> dbg_task_notify
  - >> rt_dispatch
  [Address Reference Count : 1]
  - main.o(.text)

  ### Local Symbols

  Default_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> Default_Handler
  [Called By]
  - >> Default_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  rt_init_context (Thumb, 64 bytes, Stack size 16 bytes, rt_task.o(i.rt_init_context))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_init_stack
  - >> rt_alloc_box
  [Called By]
  - >> rt_tsk_create
  - >> rt_sys_init

  _fp_digits (Thumb, 318 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_ddiv
  - >> __aeabi_dmul
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1778 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 38 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols