Static Call Graph - [.\Obj\RTX_Session1.axf]

# Static Call Graph for image .\Obj\RTX_Session1.axf

#<CALLGRAPH># ARM Linker, 5.02 [Build 28]: Last Updated: Tue Dec 25 19:02:01 2012

### Maximum Stack Usage = 88 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ InitHAL ⇒ SystemInit ⇒ __aeabi_dmul

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- rt_alloc_box ⇒ rt_alloc_box
- Default_Handler ⇒ Default_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - BusFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - Default_Handler from startup_stm32f10x_cl.o(.text) referenced 7 times from startup_stm32f10x_cl.o(RESET)
  - ETH_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI0_IRQHandler from hal_gpio.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - HardFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - LED_Task from rt_gpio.o(.text) referenced from main.o(.text)
  - MemManage_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - NMI_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - PendSV_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - Reset_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - SVC_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - SysTick_Handler from hal_cm3.o(.emb_text) referenced from startup_stm32f10x_cl.o(RESET)
  - TAMPER_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_cl.o(.text) referenced from startup_stm32f10x_cl.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_cl.o(.text)
  - init from main.o(.text) referenced from main.o(.text)
  - os_idle_demon from rtx_conf_cm.o(.text) referenced from rt_task.o(i.rt_sys_init)
  - rt_alloc_box from rt_membox.o(i.rt_alloc_box) referenced from hal_cm3.o(.emb_text)
  - rt_dly_wait from rt_time.o(i.rt_dly_wait) referenced from rt_gpio.o(.text)
  - rt_free_box from rt_membox.o(i.rt_free_box) referenced from hal_cm3.o(.emb_text)
  - rt_mut_release from rt_mutex.o(i.rt_mut_release) referenced from rtx_conf_cm.o(.text)
  - rt_mut_wait from rt_mutex.o(i.rt_mut_wait) referenced from rtx_conf_cm.o(.text)
  - rt_sys_init from rt_task.o(i.rt_sys_init) referenced from main.o(.text)
  - rt_tsk_create from rt_task.o(i.rt_tsk_create) referenced from main.o(.text)
  - rt_tsk_delete from rt_task.o(i.rt_tsk_delete) referenced from main.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ InitHAL ⇒ SystemInit ⇒ __aeabi_dmul
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  rt_set_PSP (Thumb, 6 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> rt_sys_init

  rt_get_PSP (Thumb, 6 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> rt_tsk_delete

  os_set_env (Thumb, 24 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> main

  _alloc_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  _free_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  SVC_Handler (Thumb, 124 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Calls]

  - >> rt_stk_check
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  PendSV_Handler (Thumb, 76 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = PendSV_Handler ⇒ rt_pop_req ⇒ rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_pop_req
  - >> rt_stk_check
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Stack]

  - Max Depth = 36
  - Call Chain = SysTick_Handler ⇒ rt_systick ⇒ rt_dec_dly ⇒ rt_put_prio
  [Calls]
  - >> rt_systick
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  OS_Tick_Handler (Thumb, 12 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)
  [Calls]

  - >> rt_systick
  - >> os_tick_irqack

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_cl.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  SystemInit (Thumb, 430 bytes, Stack size 40 bytes, system_stm32f10x_cl.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SystemInit ⇒ __aeabi_dmul
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_d2uiz
  [Called By]
  - >> InitHAL

  os_idle_demon (Thumb, 4 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Address Reference Count : 1]

  - rt_task.o(i.rt_sys_init)

  os_tmr_call (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_tmr_tick

  os_error (Thumb, 4 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_mbx_psh
  - >> rt_stk_check

  rt_init_robin (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_sys_init

  rt_chk_robin (Thumb, 2 bytes, Stack size 0 bytes, rtx_conf_cm.o(.text))
  [Called By]

  - >> rt_systick

  __user_perthread_libspace (Thumb, 26 bytes, Stack size 8 bytes, rtx_conf_cm.o(.text), UNUSED, KEPT)
  [Stack]

  - Max Depth = 8
  - Call Chain = __user_perthread_libspace
  [Calls]
  - >> rt_tsk_self

  _mutex_initialize (Thumb, 38 bytes, Stack size 8 bytes, rtx_conf_cm.o(.text), UNUSED, KEPT)
  [Stack]

  - Max Depth = 8
  - Call Chain = _mutex_initialize
  [Calls]
  - >> rt_mut_init

  _mutex_acquire (Thumb, 26 bytes, Stack size 8 bytes, rtx_conf_cm.o(.text), UNUSED, KEPT)
  [Stack]

  - Max Depth = 8
  - Call Chain = _mutex_acquire
  [Calls]
  - >> rt_tsk_self

  _mutex_release (Thumb, 22 bytes, Stack size 8 bytes, rtx_conf_cm.o(.text), UNUSED, KEPT)
  [Stack]

  - Max Depth = 8
  - Call Chain = _mutex_release
  [Calls]
  - >> rt_tsk_self

  init (Thumb, 26 bytes, Stack size 0 bytes, main.o(.text))
  [Address Reference Count : 1]

  - main.o(.text)

  main (Thumb, 32 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = main ⇒ InitHAL ⇒ SystemInit ⇒ __aeabi_dmul
  [Calls]
  - >> os_set_env
  - >> InitHAL
  - >> InitGPIO
  [Called By]
  - >> __rt_entry_main

  LED_Task (Thumb, 32 bytes, Stack size 0 bytes, rt_gpio.o(.text))
  [Calls]

  - >> LED_On
  - >> LED_Off
  [Address Reference Count : 1]
  - main.o(.text)

  InitGPIO (Thumb, 54 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> main

  EnableButtonIRQ (Thumb, 24 bytes, Stack size 0 bytes, hal_gpio.o(.text), UNUSED)

  DisableButtonIRQ (Thumb, 18 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> EXTI0_IRQHandler

  EXTI0_IRQHandler (Thumb, 24 bytes, Stack size 4 bytes, hal_gpio.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = EXTI0_IRQHandler
  [Calls]
  - >> DisableButtonIRQ
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  LED_On (Thumb, 14 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> LED_Task

  LED_Off (Thumb, 14 bytes, Stack size 0 bytes, hal_gpio.o(.text))
  [Called By]

  - >> LED_Task

  LED_Toggle (Thumb, 22 bytes, Stack size 0 bytes, hal_gpio.o(.text), UNUSED)

  InitHAL (Thumb, 8 bytes, Stack size 8 bytes, hal.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = InitHAL ⇒ SystemInit ⇒ __aeabi_dmul
  [Calls]
  - >> SystemInit
  [Called By]
  - >> main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  _init_box (Thumb, 70 bytes, Stack size 8 bytes, rt_membox.o(i._init_box))
  [Stack]

  - Max Depth = 8
  - Call Chain = _init_box
  [Called By]
  - >> rt_sys_init

  dbg_init (Thumb, 34 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_init))
  [Called By]

  - >> rt_sys_init

  dbg_task_notify (Thumb, 32 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_task_notify))
  [Called By]

  - >> rt_tsk_delete
  - >> rt_tsk_create

  dbg_task_switch (Thumb, 16 bytes, Stack size 0 bytes, hal_cm3.o(i.dbg_task_switch))
  [Called By]

  - >> rt_switch_req

  os_tick_init (Thumb, 32 bytes, Stack size 0 bytes, rt_system.o(i.os_tick_init))
  [Called By]

  - >> rt_sys_init

  os_tick_irqack (Thumb, 2 bytes, Stack size 0 bytes, rt_system.o(i.os_tick_irqack), UNUSED)
  [Called By]

  - >> OS_Tick_Handler

  rt_alloc_box (Thumb, 26 bytes, Stack size 0 bytes, rt_membox.o(i.rt_alloc_box))
  [Calls]

  - >> rt_alloc_box
  [Called By]
  - >> rt_alloc_box
  - >> rt_init_context
  - >> rt_tsk_create
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_block (Thumb, 48 bytes, Stack size 16 bytes, rt_task.o(i.rt_block))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_put_dly
  - >> rt_get_first
  - >> rt_switch_req
  [Called By]
  - >> rt_dly_wait
  - >> rt_mut_wait

  rt_dec_dly (Thumb, 106 bytes, Stack size 16 bytes, rt_list.o(i.rt_dec_dly))
  [Stack]

  - Max Depth = 28
  - Call Chain = rt_dec_dly ⇒ rt_put_prio
  [Calls]
  - >> rt_put_prio
  [Called By]
  - >> rt_systick

  rt_dispatch (Thumb, 60 bytes, Stack size 16 bytes, rt_task.o(i.rt_dispatch))
  [Stack]

  - Max Depth = 28
  - Call Chain = rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_put_rdy_first
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_switch_req
  [Called By]
  - >> rt_tsk_delete
  - >> rt_tsk_create
  - >> rt_mut_release

  rt_dly_wait (Thumb, 6 bytes, Stack size 0 bytes, rt_time.o(i.rt_dly_wait))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_dly_wait ⇒ rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_block
  [Address Reference Count : 1]
  - rt_gpio.o(.text)

  rt_evt_psh (Thumb, 72 bytes, Stack size 8 bytes, rt_event.o(i.rt_evt_psh))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_evt_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  [Called By]
  - >> rt_pop_req

  rt_free_box (Thumb, 32 bytes, Stack size 0 bytes, rt_membox.o(i.rt_free_box))
  [Called By]

  - >> rt_tmr_tick
  - >> rt_tsk_delete
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_get_first (Thumb, 40 bytes, Stack size 0 bytes, rt_list.o(i.rt_get_first))
  [Called By]

  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_systick
  - >> rt_pop_req
  - >> rt_dispatch
  - >> rt_block
  - >> rt_mut_release

  rt_init_stack (Thumb, 70 bytes, Stack size 8 bytes, hal_cm3.o(i.rt_init_stack))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_init_stack
  [Called By]
  - >> rt_init_context

  rt_mbx_psh (Thumb, 188 bytes, Stack size 24 bytes, rt_mailbox.o(i.rt_mbx_psh))
  [Stack]

  - Max Depth = 36
  - Call Chain = rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  - >> os_error
  [Called By]
  - >> rt_pop_req

  rt_mut_init (Thumb, 16 bytes, Stack size 0 bytes, rt_mutex.o(i.rt_mut_init), UNUSED, KEPT)
  [Called By]

  - >> _mutex_initialize

  rt_mut_release (Thumb, 164 bytes, Stack size 32 bytes, rt_mutex.o(i.rt_mut_release))
  [Stack]

  - Max Depth = 60
  - Call Chain = rt_mut_release ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  [Address Reference Count : 1]
  - rtx_conf_cm.o(.text)

  rt_mut_wait (Thumb, 96 bytes, Stack size 16 bytes, rt_mutex.o(i.rt_mut_wait))
  [Stack]

  - Max Depth = 40
  - Call Chain = rt_mut_wait ⇒ rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_resort_prio
  - >> rt_put_prio
  - >> rt_block
  [Address Reference Count : 1]
  - rtx_conf_cm.o(.text)

  rt_pop_req (Thumb, 106 bytes, Stack size 16 bytes, rt_system.o(i.rt_pop_req))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_pop_req ⇒ rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_put_rdy_first
  - >> rt_get_first
  - >> rt_switch_req
  [Called By]
  - >> PendSV_Handler

  rt_put_dly (Thumb, 68 bytes, Stack size 8 bytes, rt_list.o(i.rt_put_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_put_dly
  [Called By]
  - >> rt_block

  rt_put_prio (Thumb, 54 bytes, Stack size 12 bytes, rt_list.o(i.rt_put_prio))
  [Stack]

  - Max Depth = 12
  - Call Chain = rt_put_prio
  [Called By]
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_dec_dly
  - >> rt_resort_prio
  - >> rt_dispatch
  - >> rt_mut_wait
  - >> rt_mut_release

  rt_put_rdy_first (Thumb, 14 bytes, Stack size 0 bytes, rt_list.o(i.rt_put_rdy_first))
  [Called By]

  - >> rt_systick
  - >> rt_pop_req
  - >> rt_dispatch

  rt_resort_prio (Thumb, 46 bytes, Stack size 8 bytes, rt_list.o(i.rt_resort_prio))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_resort_prio ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_list
  - >> rt_put_prio
  [Called By]
  - >> rt_mut_wait

  rt_rmv_dly (Thumb, 40 bytes, Stack size 8 bytes, rt_list.o(i.rt_rmv_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_rmv_dly
  [Called By]
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_tsk_delete
  - >> rt_mut_release

  rt_rmv_list (Thumb, 44 bytes, Stack size 0 bytes, rt_list.o(i.rt_rmv_list))
  [Called By]

  - >> rt_resort_prio
  - >> rt_tsk_delete

  rt_sem_psh (Thumb, 46 bytes, Stack size 8 bytes, rt_semaphore.o(i.rt_sem_psh))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_sem_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_put_prio
  - >> rt_get_first
  [Called By]
  - >> rt_pop_req

  rt_stk_check (Thumb, 28 bytes, Stack size 0 bytes, rt_system.o(i.rt_stk_check))
  [Calls]

  - >> os_error
  [Called By]
  - >> PendSV_Handler
  - >> SVC_Handler
  - >> rt_tsk_delete

  rt_switch_req (Thumb, 30 bytes, Stack size 0 bytes, rt_task.o(i.rt_switch_req))
  [Calls]

  - >> dbg_task_switch
  [Called By]
  - >> rt_systick
  - >> rt_pop_req
  - >> rt_dispatch
  - >> rt_block

  rt_sys_init (Thumb, 266 bytes, Stack size 32 bytes, rt_task.o(i.rt_sys_init))
  [Stack]

  - Max Depth = 84
  - Call Chain = rt_sys_init ⇒ rt_tsk_create ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_set_PSP
  - >> os_tick_init
  - >> dbg_init
  - >> _init_box
  - >> rt_init_context
  - >> rt_tsk_create
  - >> rt_init_robin
  [Address Reference Count : 1]
  - main.o(.text)

  rt_systick (Thumb, 48 bytes, Stack size 8 bytes, rt_system.o(i.rt_systick))
  [Stack]

  - Max Depth = 36
  - Call Chain = rt_systick ⇒ rt_dec_dly ⇒ rt_put_prio
  [Calls]
  - >> rt_tmr_tick
  - >> rt_dec_dly
  - >> rt_put_rdy_first
  - >> rt_get_first
  - >> rt_switch_req
  - >> rt_chk_robin
  [Called By]
  - >> OS_Tick_Handler
  - >> SysTick_Handler

  rt_tmr_tick (Thumb, 56 bytes, Stack size 16 bytes, rt_timer.o(i.rt_tmr_tick))
  [Stack]

  - Max Depth = 16
  - Call Chain = rt_tmr_tick
  [Calls]
  - >> rt_free_box
  - >> os_tmr_call
  [Called By]
  - >> rt_systick

  rt_tsk_create (Thumb, 126 bytes, Stack size 24 bytes, rt_task.o(i.rt_tsk_create))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_tsk_create ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_alloc_box
  - >> dbg_task_notify
  - >> rt_dispatch
  - >> rt_init_context
  [Called By]
  - >> rt_sys_init
  [Address Reference Count : 1]
  - main.o(.text)

  rt_tsk_delete (Thumb, 162 bytes, Stack size 24 bytes, rt_task.o(i.rt_tsk_delete))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_tsk_delete ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_stk_check
  - >> rt_rmv_list
  - >> rt_rmv_dly
  - >> rt_get_PSP
  - >> rt_free_box
  - >> dbg_task_notify
  - >> rt_dispatch
  [Address Reference Count : 1]
  - main.o(.text)

  rt_tsk_self (Thumb, 12 bytes, Stack size 0 bytes, rt_task.o(i.rt_tsk_self), UNUSED, KEPT)
  [Called By]

  - >> _mutex_release
  - >> _mutex_acquire
  - >> __user_perthread_libspace

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> SystemInit

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt))
  [Called By]

  - >> SystemInit

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> SystemInit

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf), UNUSED)
  [Called By]

  - >> _dmul
  - >> _dfixu

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _dmul

  ### Local Symbols

  Default_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> Default_Handler
  [Called By]
  - >> Default_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  rt_init_context (Thumb, 64 bytes, Stack size 16 bytes, rt_task.o(i.rt_init_context))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_init_stack
  - >> rt_alloc_box
  [Called By]
  - >> rt_tsk_create
  - >> rt_sys_init

  ### Undefined Global Symbols