

Center: 

When emulation started, the trace buffer keeps refreshing in the first half of the trace buffer until matching the set trigger. While matching, cycles will fill in the other half of trace buffer. While trace buffer is full, emulation is stopped.
