
       Flash Parts Supported by EPI Flash Utility  v2.5.2.7

                    Sept 9, 2004



     SUPPORTED       DATA BUS   EQUIVALENT PART TO USE
    FLASH PARTS       WIDTH       IN FLASH UTILITY

AMD
    Am29DL161DB         x8      (USE Am29DL163DB x8)
    Am29DL161DT         x8      (USE Am29DL163DT x8)
    Am29DL161DB         x16     (USE Am29DL163DB x16)
    Am29DL161DT         x16     (USE Am29DL163DT x16)

    Am29DL162DB         x8      (USE Am29DL163DB x8)
    Am29DL162DT         x8      (USE Am29DL163DT x8)
    Am29DL162DB         x16     (USE Am29DL163DB x16)
    Am29DL162DT         x16     (USE Am29DL163DT x16)

    Am29DL163DB         x8
    Am29DL163DT         x8
    Am29DL163DB         x16
    Am29DL163DT         x16

    Am29DL164DB         x8      (USE Am29DL163DB x8)
    Am29DL164DT         x8      (USE Am29DL163DT x8)
    Am29DL164DB         x16     (USE Am29DL163DB x16)
    Am29DL164DT         x16     (USE Am29DL163DT x16)

    Am29DL322DB         x8      (USE Am29LV320DB x8)
    Am29DL322DT         x8      (USE Am29LV320DT x8)
    Am29DL322DB         x16     (USE Am29LV320DB x16)
    Am29DL322DT         x16     (USE Am29LV320DT x16)

    Am29DL323DB         X8      (USE Am29LV320DB x8)
    Am29DL323DT         X8      (USE Am29LV320DT x8)
    Am29DL323DB         x16     (USE Am29LV320DB x16)
    Am29DL323DT         x16     (USE Am29LV320DT x16)

    Am29DL324DB         x8      (USE Am29LV320DB x8)
    Am29DL324DT         x8      (USE Am29LV320DT x8)
    Am29DL324DB         x16     (USE Am29LV320DB x16)
    Am29DL324DT         x16     (USE Am29LV320DT x16)

    Am29DL322GB         x8      (USE Am29LV320DB x8)
    Am29DL322GT         x8      (USE Am29LV320DT x8)
    Am29DL322GB         x16     (USE Am29LV320DB x16)
    Am29DL322GT         x16     (USE Am29LV320DT x16)

    Am29DL323GB         X8      (USE Am29LV320DB x8)
    Am29DL323GT         X8      (USE Am29LV320DT x8)
    Am29DL323GB         x16     (USE Am29LV320DB x16)
    Am29DL323GT         x16     (USE Am29LV320DT x16)

    Am29DL324GB         x8      (USE Am29LV320DB x8)
    Am29DL324GT         x8      (USE Am29LV320DT x8)
    Am29DL324GB         x16     (USE Am29LV320DB x16)
    Am29DL324GT         x16     (USE Am29LV320DT x16)

    Am29DL640G          x8
    Am29DL640G          x16

    Am29F040B           x8
    Am29F080B           x8

    Am29LV040B          x8      (USE Am29F040B x8)
    Am29LV033C          x8
    Am29LV065D          x8      (USE Am29LV640MH x8)


    Am29LV160BB         x8
    Am29LV160BT         x8
    Am29LV160BB         x16
    Am29LV160BT         x16

    Am29LV800BB         x8
    Am29LV800BT         x8
    Am29LV800BB         x16
    Am29LV800BT         x16

    Am29LV400BB         x8
    Am29LV400BB         x16
    Am29LV400BT    x8   (NOT SUPPORTED, TBA)
    Am29LV400BT    x16  (NOT SUPPORTED, TBA)

    Am29LV160DB         x8      (USE Am29LV160BB x8)
    Am29LV160DT         x8      (USE Am29LV160BT x8)
    Am29LV160DB         x16     (USE Am29LV160BB x16)
    Am29LV160DT         x16     (USE Am29LV160BT x16)

    Am29LV320DB         x8
    Am29LV320DT         x8
    Am29LV320DB         x16
    Am29LV320DT         x16

    Am29LV128MH    x8   (NOT SUPPORTED, TBA)
    Am29LV128MH         x16     (aka Am29LV128MH/L, Am29LV128ML)
    Am29LV256MH    x8   (NOT SUPPORTED, TBA)
    Am29LV256MH         x16     (aka Am29LV256MH/L, Am29LV256ML)
    Am29LV640MH         x8      (aka Am29LV640MH/L, Am29LV640ML)
    Am29LV640MH         x16     (USE Am29LV641MH x16)
    Am29LV641MH         x16

    Am29LV320MB         x8      (USE Am29LV320DB x8)
    Am29LV320MT         x8      (USE Am29LV320DT x8)
    Am29LV320MB         x16     (USE Am29LV320DB x16)
    Am29LV320MT         x16     (USE Am29LV320DT x16)

    Am29LV640MB         x8
    Am29LV640MT         x8
    Am29LV640MB         x16
    Am29LV640MT         x16

    Am29PDL127H         x16

    Am45DL3208GB        x8      (USE Am29LV320DB x8)
    Am45DL3208GT        x8      (USE Am29LV320DT x8)
    Am45DL3208GB        x16     (USE Am29LV320DB x16)
    Am45DL3208GT        x16     (USE Am29LV320DT x16)


NOTES:  (H/L) These parts are identical for flash utility.


Intel
    28F008B3B           x8
    28F008B3T           x8
    28F800B3B      x16  (NOT SUPPORTED, TBA)
    28F800B3T      x16  (NOT SUPPORTED, TBA)
    28F016B3T           x8
    28F016B3B      x8   (NOT SUPPORTED, TBA)
    28F160B3B      x16  (NOT SUPPORTED, TBA)
    28F160B3T      x16  (NOT SUPPORTED, TBA)
    28F320B3B           x16
    28F320B3T           x16
    28F640B3B           x16
    28F640B3T      x16  (NOT SUPPORTED, TBA)


    28F160C3B           x16
    28F160C3T      x16  (NOT SUPPORTED, TBA)
    28F320C3B           x16
    28F320C3T           x16
    28F640C3B           x16
    28F640C3T      x16  (NOT SUPPORTED, TBA)


    28F320J3            x8
    28F320J3            x16
    28F640J3            x8
    28F640J3            x16
    28F128J3            x8
    28F128J3            x16

    28F640K3            x16     (USE 28F640J3 x16)
    28F128K3            x16     (USE 28F128J3 x16)
    28F256K3            x16

    28F640K18           x16     (USE 28F640J3 x16)
    28F128K18           x16     (USE 28F128J3 x16)
    28F256K18           x16     (USE 28F256K3 x16)

    28F640L18B          x16
    28F640L18T          x16
    28F128L18B          x16
    28F128L18T          x16
    28F256L18B          x16
    28F256L18T          x16

    28F640L30B          x16     (USE 28F640L18B x16)
    28F640L30T          x16     (USE 28F640L18T x16)
    28F128L30B          x16     (USE 28F128L18B x16)
    28F128L30T          x16     (USE 28F128L18T x16)
    28F256L30B          x16     (USE 28F256L18B x16)
    28F256L30T          x16     (USE 28F256L18T x16)

    28F008S3       x8   (NOT SUPPORTED, TBA)
    28F160S3       x8   (NOT SUPPORTED, TBA)
    28F160S3            x16     (USE 28F160S5 x16)
    28F008S5       x8   (NOT SUPPORTED, TBA)
    28F160S5       x8   (NOT SUPPORTED, TBA)
    28F160S5            x16

    28F640W18B          x16
    28F640W18T          x16
    28F640W30B          x16     (USE 28F640W18B x16)
    28F640W30T          x16     (USE 28F640W18T x16)

    28F320W18B      x16  (NOT SUPPORTED, TBA)
    28F320W18T      x16  (NOT SUPPORTED, TBA)
    28F640W18B          x16
    28F640W18T          x16
    28F128W18B      x16  (NOT SUPPORTED, TBA)
    28F128W18T      x16  (NOT SUPPORTED, TBA)

    28F320W30B      x16  (NOT SUPPORTED, TBA)
    28F320W30T      x16  (NOT SUPPORTED, TBA)
    28F640W30B          x16     (USE 28F640W18B x16)
    28F640W30T          x16     (USE 28F640W18T x16)
    28F128W30B      x16  (NOT SUPPORTED, TBA)
    28F128W30T      x16  (NOT SUPPORTED, TBA)


ATMEL
    AT49BV1604AB        x16
    AT49BV1604AT        x16
    AT49BV1614AB        x8
    AT49BV1614AT        x8
    AT49BV1614TB        x16
    AT49BV1614TT        x16

    AT49BV162A          x8      (USE Am29DL163DB x8)
    AT49BV162A          x16     (USE Am29DL163DB x16)
    AT49BV162AT         x8      (USE Am29DL163DT x8)
    AT49BV162AT         x16     (USE Am29DL163DT x16)
    
    AT49BV322A          x8      (USE Am29LV320DB x8)
    AT49BV322AT         x8      (USE Am29LV320DT x8)
    AT49BV322A          x16     (USE Am29LV320DB x16)
    AT49BV322AT         x16     (USE Am29LV320DT x16)

    AT49BV4096A         x16     (NOTE: Part has non-standard sectors sizes)
    AT49LV4096A         x16     (USE AT49BV4096A x16)

    AT29LV1024          x16


Fujitsu
    MBM29LV160B         x8      (USE Am29LV160BB x8)
    MBM29LV160T         x8      (USE Am29LV160BT x8)
    MBM29LV160B         x16     (USE Am29LV160BB x16)
    MBM29LV160T         x16     (USE Am29LV160BT x16)


Micronix (MXIC)
    MX29LV320B          x8      (USE Am29LV320DB x8)
    MX29LV320T          x8      (USE Am29LV320DT x8)


ST Microelectronics
    M29DW640D           x8      (USE Am29DL640G x8)
    M29DW640D           x16     (USE Am29DL640G x16)

    M29DW323DB          x8      (USE Am29LV320DB x8)
    M29DW323DB          x16     (USE Am29LV320DB x16)
    M29DW323DT          x8      (USE Am29LV320DT x8)
    M29DW323DT          x16     (USE Am29LV320DT x16)

    M30LW128D           x8      (USE 28F640J3 x8, 2 Devices in series)
    M30LW128D           x16     (USE 28F640J3 x16, 2 Devices in series)

    M58LW064D           x8      (USE 28F640J3 x8)
    M58LW064D           x16     (USE 28F640J3 x16)


Silicon Storage Technology (SST)
    SST39LF200A         x16
    SST39LF400A         x16
    SST39LF010          x8      (USE SST39VF010 x8)
    SST39LF016          x8      (USE SST39VF016 x8)
    SST39VF1601         x16
    SST39VF010          x8
    SST39VF016          x8
    SST39VF160          x16
    SST39VF1602         x16     (USE SST39VF1601 x16)
    SST39VF3201         x16     (USE SST39VF3202 x16)
    SST39VF3202         x16


Toshiba
    TC58FVT160AFT       x8      (USE Am29LV160BT x8)
    TC58FVB160AFT       x8      (USE Am29LV160BB x8)
    TC58FVT160AFT       x16     (USE Am29LV160BT x16)
    TC58FVB160AFT       x16     (USE Am29LV160BB x16)

    TC58FVB321FT        x8      (USE Am29LV320DB x8)
    TC58FVT321FT        x8      (USE Am29LV320DT x8)
    TC58FVB321FT        x16     (USE Am29LV320DB x16)
    TC58FVT321FT        x16     (USE Am29LV320DT x16)

    TC58FVB641     x8      (NOT SUPPORTED, TBA - USE Am29LV640MB x8)
    TC58FVT641     x8      (NOT SUPPORTED, TBA - USE Am29LV640MT x8)
    TC58FVB641          x16     (USE Am29LV640MB x16)
    TC58FVT641          x16     (USE Am29LV640MT x16)
    TC58FVB641                  (aka TC58FVB641XB, TC58FVB641FT)
    TC58FVT641                  (aka TC58FVT641XB, TC58FVT641FT)

    TC58FVM6B2A     x8      (NOT SUPPORTED, TBA - USE Am29LV640MB x8)
    TC58FVM6T2A     x8      (NOT SUPPORTED, TBA - USE Am29LV640MT x8)
    TC58FVM6B2A          x16     (USE Am29LV640MB x16)
    TC58FVM6T2A          x16     (USE Am29LV640MT x16)
    TC58FVM6B2A         (aka TC58FVM6B2AFT, TC58FVM6B2AXB, TC58FVM6B2ATG)
    TC58FVM6T2A         (aka TC58FVM6T2AFT, TC58FVM6T2AXB, TC58FVM6T2ATG)

NOTE:   (Toshiba Hidden ROM area NOT supported)


Winbond
    W19B320SB           x8      (USE Am29LV320DB x8)
    W19B320ST           x8      (USE Am29LV320DT x8)
    W19B320SB           x16     (USE Am29LV320DB x16)
    W19B320ST           x16     (USE Am29LV320DT x16)

    W19L320SB           x8      (USE Am29LV320DB x8)
    W19L320ST           x8      (USE Am29LV320DT x8)
    W19L320SB           x16     (USE Am29LV320DB x16)
    W19L320ST           x16     (USE Am29LV320DT x16)


----------------------------------------------------------------------------

            These NOTES pertain to ALL flash parts.

  (T/B) T = Boot Top device, B = Boot Bottom device.
        These parts are unique for the flash utility. These parts will be
        found in the same document (data sheet) as the supported part.

  (TBA) These parts can be added with near zero effort.

  (USE) These parts are identical for the flash utility. These parts may or
        may not be found in the same document (data sheet) as the supported
        part.

  (aka) These parts are identical for flash utility. These parts in most cases
        will be found in the same document (data sheet) as the supported part.
