<?xml version="1.0" standalone="no" ?>
<!-- Hitool Project File -->
<Project name="./RelRom/##project.elf" type="0" ExtMakefile="" Mask="0" Remote="false" RemoteServer="" RemotePort="0" RemoteRoot="">
    <CFG name="Debug Rom" />
    <ProjectType name="Executable" output="elf">
        <CFG name="C Source" extension="c;cpp;cxx;cc" output="o" tool="CC" Application="arm-elf-gcc" pre="false" flag="CFLAGS" cmd='@$(CC) -c -o &quot;$@&quot; &quot;$&lt;&quot; $(CFLAGS) $(SYS_INCLUDE)' />
        <CFG name="Assembler Source" extension="asm;s" output="o" tool="AS" Application="arm-elf-as" pre="false" flag="ASFLAGS" cmd='@$(CC) -c -o &quot;$@&quot; &quot;$&lt;&quot; $(ASFLAGS)' />
        <CFG name="Object File" extension="obj;o;a;lib" output="elf" tool="LD" Application="arm-elf-ld" pre="false" flag="LDFLAGS" cmd="@$(CC) -o $@ $(STARTUP) $(OBJECTS) $(LDFLAGS) $(SYS_LIB)" />
    </ProjectType>
    <Configurations>
        <CFG name="Debug Ram">
            <Debug name="./DbgRam/##project.elf" path="./DbgRam" argu="" output="" cmdfile="" cmdfile_prompt="true" />
            <Tool name="CC" base="-gstabs+ -O0 -D_DEBUG -Wall" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O0 -I. -D_DEBUG -Wall -gstabs+ " />
            <Tool name="AS" base="-Wa,--gstabs" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -Wa,--gstabs " />
            <Tool name="LD" base="-T $(LD_SCRIPT) -Wl,--defsym -Wl,__stack_base=$(TOPMEMORY) -static " current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_ram.ld -Ttext 0x1000000 -Tdata 0x1080000 -Tbss 0x10f0000 -Wl,--defsym -Wl,__stack_base=0x1200000 -static " />
            <Tool name="LD_SCRIPT" base="ldscript_ram.ld" current="ldscript_ram.ld" />
            <Tool name="TARGET" base="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian" />
            <General name="##project.elf" path="./DbgRam" />
            <Post>
                <CFG name="" />
            </Post>
            <Pre>
                <CFG name="" />
            </Pre>
        </CFG>
        <CFG name="Debug Rom">
            <Debug name="./DbgRom/##project.elf" path="./DbgRom" argu="" output="" cmdfile="" cmdfile_prompt="true" />
            <Tool name="CC" base="-gstabs+ -O0 -D_DEBUG -Wall" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O0 -I. -D_DEBUG -Wall -gstabs+ " />
            <Tool name="AS" base="-Wa,--gstabs" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -Wa,--gstabs " />
            <Tool name="LD" base="-T $(LD_SCRIPT) -Wl,--defsym -Wl,__stack_base=$(TOPMEMORY)" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_rom.ld -Ttext 0x1000 -Tdata 0x101a000 -Tbss 0x1030000 -Wl,--defsym -Wl,__stack_base=0x1074000 " />
            <Tool name="LD_SCRIPT" base="ldscript_rom.ld" current="ldscript_rom.ld" />
            <Tool name="TARGET" base="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " />
            <General name="##project.elf" path="./DbgRom" />
            <Post>
                <CFG name="arm-elf-objcopy -O binary -R .comment -R .note -S $(OUTPUT_NAME) $(basename $(OUTPUT_NAME)).bin" />
            </Post>
            <Pre>
                <CFG name="" />
            </Pre>
        </CFG>
        <CFG name="Release Ram">
            <Debug name="./RelRam/##project.elf" path="./RelRam" argu="" output="" cmdfile="" cmdfile_prompt="true" />
            <Tool name="CC" base="-O2" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O2 -I. -gdwarf-2 " />
            <Tool name="AS" base="-Os" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian " />
            <Tool name="LD" base="-T $(LD_SCRIPT) -static -Wl,--defsym -Wl,__stack_base=$(TOPMEMORY)" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_ram.ld -Ttext 0x1000000 -Tdata 0x1080000 -Tbss 0x10f0000 -Wl,--defsym -Wl,__stack_base=0x1200000 -static " />
            <Tool name="LD_SCRIPT" base="ldscript_ram.ld" current="ldscript_ram.ld" />
            <Tool name="TARGET" base="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " />
            <General name="##project.elf" path="./RelRam" />
            <Post>
                <CFG name="" />
            </Post>
            <Pre>
                <CFG name="" />
            </Pre>
        </CFG>
        <CFG name="Release Rom">
            <Debug name="./RelRom/##project.elf" path="./RelRom" argu="" output="" cmdfile="" cmdfile_prompt="true" />
            <Tool name="CC" base="-O2" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O2 -I. -gdwarf-2 " />
            <Tool name="AS" base="-Os" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian " />
            <Tool name="LD" base="-T $(LD_SCRIPT) -Wl,--defsym -Wl,__stack_base=$(TOPMEMORY)" current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_rom.ld -Ttext 0x1000 -Tdata 0x101a000 -Tbss 0x1030000 -Wl,--defsym -Wl,__stack_base=0x1074000 " />
            <Tool name="LD_SCRIPT" base="ldscript_rom.ld" current="ldscript_rom.ld" />
            <Tool name="TARGET" base="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " current="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian  " />
            <General name="##project.elf" path="./RelRom" />
            <Post>
                <CFG name="arm-elf-objcopy -O binary -R .comment -R .note -S $(OUTPUT_NAME) $(basename $(OUTPUT_NAME)).bin" />
            </Post>
            <Pre>
                <CFG name="" />
            </Pre>
        </CFG>
    </Configurations>
    <Target>
        <LinkOrder name="" />
        <Group name="Source Files" filter="c;cpp;cxx;cc;S;s">
            <Source name="hw_init.S">
                <exclude config="Debug Ram" value="1" />
                <Tool config="Debug Ram" name="CC" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O0 -I. -D_DEBUG -Wall -gstabs+ " nglobal="" />
                <Tool config="Debug Ram" name="AS" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -Wa,--gstabs " nglobal="" />
                <Tool config="Debug Ram" name="LD" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_ram.ld -Ttext 0x1000000 -Tdata 0x1080000 -Tbss 0x10f0000 -Wl,--defsym -Wl,__stack_base=0x1200000 -static " nglobal="" />
                <exclude config="Release Rom" value="0" />
                <Tool config="Release Rom" name="CC" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O2 -I. -gdwarf-2 " nglobal="" />
                <Tool config="Release Rom" name="AS" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian " nglobal="" />
                <Tool config="Release Rom" name="LD" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_rom.ld -Ttext 0x1000 -Tdata 0x101a000 -Tbss 0x1030000 -Wl,--defsym -Wl,__stack_base=0x1074000 " nglobal="" />
                <exclude config="Debug Rom" value="0" />
                <Tool config="Debug Rom" name="CC" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O0 -I. -D_DEBUG -Wall -gstabs+ " nglobal="" />
                <Tool config="Debug Rom" name="AS" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -Wa,--gstabs " nglobal="" />
                <Tool config="Debug Rom" name="LD" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_rom.ld -Ttext 0x1000 -Tdata 0x101a000 -Tbss 0x1030000 -Wl,--defsym -Wl,__stack_base=0x1074000 " nglobal="" />
                <exclude config="Release Ram" value="1" />
                <Tool config="Release Ram" name="CC" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -O2 -I. -gdwarf-2 " nglobal="" />
                <Tool config="Release Ram" name="AS" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian " nglobal="" />
                <Tool config="Release Ram" name="LD" command="-mcpu=arm7tdmi -mapcs-32 -mlittle-endian -T ldscript_ram.ld -Ttext 0x1000000 -Tdata 0x1080000 -Tbss 0x10f0000 -Wl,--defsym -Wl,__stack_base=0x1200000 -static " nglobal="" />
            </Source>
            <Source name="uart_ev4510.c" />
            <Source name="main.c" />
        </Group>
        <Group name="Header Files" filter="h;hpp;hxx;inc;inl" />
        <Group name="Lib Files" filter="obj;o;a;lib" />
    </Target>
    <FileMap>
        <CFG name="C Source" extension="c;cpp;cxx;cc" output="o" tool="CC" Application="arm-elf-gcc" pre="false" />
        <CFG name="Assembler Source" extension="asm;s" output="o" tool="AS" Application="arm-elf-as" pre="false" />
        <CFG name="Object File" extension="obj;o;a;lib" output="elf" tool="LD" Application="arm-elf-ld" pre="false" />
    </FileMap>
    <path />
</Project>
