----------------------------------------------------------------
		GNU Examples in JediView for ARM
 
		(c)  JediView Systems, Inc.
 ----------------------------------------------------------------
In this directory you can see three examples built by GNU compiler:
(1) Prime_arm;
(2) Prime_inter;
(3) C++.

(1)Prime_arm
There are seven files in this directory:
Prime1.c, prime2.c and prime3.c are the C source files. The target files  Ev40.elf, EV44B0II.elf, EV2500.elf and EV4510.elf, which can be loaded and run in an evaluation board.

(2)Prime_inter
There are seven files in this directory:
Prime1.c, prime2.c and prime3.c are the C source files. The target files  Ev40.elf, EV44B0II.elf, EV2500.elf and EV4510.elf, which can be loaded and run in an evaluation board.

(3)C++
There are seven files in this directory
demo.cpp is a c++ file. base.h and attac.h are the header files used by demo.cpp.  The target files  Ev40.elf, EV44B0II.elf, EV2500.elf and EV4510.elf, which can be loaded and run in an evaluation board.

If you load the sample of EV40, the correlated of initial_File is \JediView.arm\cfg\atmel_mem.inc
If you load the sample of EV4510, the correlated of initial_File is \JediView.arm\cfg\ev4510.inc
If you load the sample of EV44B0, the correlated of initial_File is \JediView.arm\cfg\Ev44B0.inc
If you load the sample of EV2500, the correlated of initial_File is \JediView.arm\cfg\ini_smdk2510.inc.inc