<SETUP CpuVendor="Samsung" CpuChip="S3C2410X" FlashVendor="Intel" FlashChip="28F800B3-B" RamAddress="0x30000000" RamSize="0x400000" NANDFlash="0x1" FlashAddress="0x0" FlashSize="0x100000" CpuType="ARM920T" CpuFamily="ARM" Register7="0x6" ManufacturersCode="0X0089" DeviceID="0X8893" INIFile="" FailMask="0x0" CpuEndian="Little" LoadFileLE="arm7.bin" LoadFileBE="arm7be.bin" Regcount="0x2f" Seccount="0x17" FlashWidth="0x8" FlashChipsPerSector="0x1">
    <Regcount Regcount="0x2f">
        <Sim Register="0x53000000" Address="0x53000000" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0x4a000008" Address="0x4a000008" Value="0xffffffff" Default="0x0" Width="32" />
        <Sim Register="0x4a00001c" Address="0x4a00001c" Value="0x000003ff" Default="0x0" Width="32" />
        <Sim Register="0x56000050" Address="0x56000050" Value="0x000055aa" Default="0x0" Width="32" />
        <Sim Register="0x56000058" Address="0x56000058" Value="0x000000ff" Default="0x0" Width="32" />
        <Sim Register="0x4c000014" Address="0x4c000014" Value="0x00000003" Default="0x0" Width="32" />
        <Sim Register="0x4c000000" Address="0x4c000000" Value="0x00ffffff" Default="0x0" Width="32" />
        <Sim Register="0x4c000004" Address="0x4c000004" Value="0x000a1031" Default="0x0" Width="32" />
        <Sim Register="0x4c000008" Address="0x4c000008" Value="0x00048032" Default="0x0" Width="32" />
        <Sim Register="control" Address="0xffffffff" Value="0xc0001078" Default="0x0" Width="32" />
        <Sim Register="0x48000000" Address="0x48000000" Value="0x2211d120" Default="0x0" Width="32" />
        <Sim Register="0x48000004" Address="0x48000004" Value="0x00000700" Default="0x0" Width="32" />
        <Sim Register="0x48000008" Address="0x48000008" Value="0x00000700" Default="0x0" Width="32" />
        <Sim Register="0x4800000c" Address="0x4800000c" Value="0x00000700" Default="0x0" Width="32" />
        <Sim Register="0x48000010" Address="0x48000010" Value="0x00001f7c" Default="0x0" Width="32" />
        <Sim Register="0x48000014" Address="0x48000014" Value="0x00000700" Default="0x0" Width="32" />
        <Sim Register="0x48000018" Address="0x48000018" Value="0x00000700" Default="0x0" Width="32" />
        <Sim Register="0x4800001c" Address="0x4800001c" Value="0x00018005" Default="0x0" Width="32" />
        <Sim Register="0x48000020" Address="0x48000020" Value="0x00018005" Default="0x0" Width="32" />
        <Sim Register="0x48000024" Address="0x48000024" Value="0x008e0459" Default="0x0" Width="32" />
        <Sim Register="0x48000028" Address="0x48000028" Value="0x00000032" Default="0x0" Width="32" />
        <Sim Register="0x4800002c" Address="0x4800002c" Value="0x00000030" Default="0x0" Width="32" />
        <Sim Register="0x48000030" Address="0x48000030" Value="0x00000030" Default="0x0" Width="32" />
        <Sim Register="0x56000000" Address="0x56000000" Value="0x007fffff" Default="0x0" Width="32" />
        <Sim Register="0x56000010" Address="0x56000010" Value="0x00044555" Default="0x0" Width="32" />
        <Sim Register="0x56000018" Address="0x56000018" Value="0x000007ff" Default="0x0" Width="32" />
        <Sim Register="0x56000020" Address="0x56000020" Value="0xaaaaaaaa" Default="0x0" Width="32" />
        <Sim Register="0x56000028" Address="0x56000028" Value="0x0000ffff" Default="0x0" Width="32" />
        <Sim Register="0x56000030" Address="0x56000030" Value="0xaaaaaaaa" Default="0x0" Width="32" />
        <Sim Register="0x56000038" Address="0x56000038" Value="0x0000ffff" Default="0x0" Width="32" />
        <Sim Register="0x56000040" Address="0x56000040" Value="0xaaaaaaaa" Default="0x0" Width="32" />
        <Sim Register="0x56000048" Address="0x56000048" Value="0x0000ffff" Default="0x0" Width="32" />
        <Sim Register="0x56000050" Address="0x56000050" Value="0x000055aa" Default="0x0" Width="32" />
        <Sim Register="0x56000058" Address="0x56000058" Value="0x000000ff" Default="0x0" Width="32" />
        <Sim Register="0x56000060" Address="0x56000060" Value="0xff95ffba" Default="0x0" Width="32" />
        <Sim Register="0x56000068" Address="0x56000068" Value="0x0000ffff" Default="0x0" Width="32" />
        <Sim Register="0x56000070" Address="0x56000070" Value="0x002afaaa" Default="0x0" Width="32" />
        <Sim Register="0x56000078" Address="0x56000078" Value="0x000007ff" Default="0x0" Width="32" />
        <Sim Register="0x56000088" Address="0x56000088" Value="0x22222222" Default="0x0" Width="32" />
        <Sim Register="0x5600008c" Address="0x5600008c" Value="0x22222242" Default="0x0" Width="32" />
        <Sim Register="0x56000090" Address="0x56000090" Value="0x22222222" Default="0x0" Width="32" />
        <Sim Register="0x50000008" Address="0x50000008" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0x5000000c" Address="0x5000000c" Value="0x00000000" Default="0x0" Width="32" />
        <Sim Register="0x50000000" Address="0x50000000" Value="0x00000003" Default="0x0" Width="32" />
        <Sim Register="0x50000004" Address="0x50000004" Value="0x00000245" Default="0x0" Width="32" />
        <Sim Register="0x50000028" Address="0x50000028" Value="0x0000001a" Default="0x0" Width="32" />
        <Sim Register="0x4e000000" Address="0x4e000000" Value="0x0000e841" Default="0x0" Width="0x0" />
    </Regcount>
    <Seccount Seccount="0x17">
        <Sector1 Sector="1" Size="8192" />
        <Sector9 Sector="9" Size="65536" />
    </Seccount>
    <CommandType name="INTEL:8/16">
        <type name="INTEL:8/16" />
    </CommandType>
    <Param FlashStart="0x200000" FileStart="0x0" FileEnd="0x1a2cfff" />
    <Nand addrEnCE="0x4e000000" maskEnCE="0x800" valEnCE="0x0" addrDisCE="0x4e000000" maskDisCE="0x800" valDisCE="0x1" addrStat="0x4e000010" maskStat="0x1" valStat="0x1" cmdPort="0x4e000004" addrPort="0x4e000008" dataPort="0x4e00000c" />
</SETUP>
